<?xml version="1.0" encoding="utf-8"?>
<!DOCTYPE eagle SYSTEM "eagle.dtd">
<eagle version="7.6.0">
<drawing>
<library>
<description>&lt;b&gt;PCB Matrix Packages&lt;/b&gt;&lt;p&gt;</description>
<packages>
<package name="SMA-F-S-TH">
</package>
<package name="SMA-F-S-EDGE">
</package>
<package name="TP_1X1">
<description>&lt;b&gt;Test Pad&lt;/b&gt; Square 1mm x 1mm</description>
</package>
<package name="HRS_UFL">
<description>&lt;b&gt;Hirose U.FL SMT&lt;/b&gt;</description>
</package>
<package name="QFN16_3X3">
</package>
<package name="AMPHENOL_SIM">
</package>
<package name="FTM-110-XX-XX-DV-S">
<description>&lt;b&gt;PCB Libraries Package&lt;b&gt;</description>
</package>
<package name="FTM-105-XX-XX-DV-S">
<description>&lt;b&gt;PCB Matrix Packages&lt;/b&gt;&lt;p&gt;</description>
</package>
<package name="FTSH-105-01-XXX-DV-K">
<description>TERMINAL STRIP, .050 inch(1.27mm) PITCH, 10 PINS, KEYED</description>
</package>
<package name="TQFP44">
<description>&lt;b&gt;Thin Quad Flat Pack&lt;/b&gt;&lt;p&gt;
package type TQ</description>
</package>
<package name="HC73">
</package>
<package name="MNR35">
</package>
<package name="SOT223-6">
<description>SOT223-6 ass found in TPS736xx data sheet</description>
</package>
<package name="QFN24_4X4">
</package>
<package name="NV08C-CSM">
</package>
<package name="JACK2.5_SJ-2523">
</package>
<package name="BA2023-ND">
<description>Footprint taken from BA2032/datasheet.pdf  6/27/08

Memory Protection Devices, Inc</description>
</package>
<package name="MOLEX_MCX_V">
</package>
<package name="0603">
</package>
<package name="AISC0402">
<description>AISC-0402 inductor footprint</description>
</package>
<package name="TSSOP20">
</package>
<package name="TSSOP8">
</package>
<package name="TSSOP16">
</package>
<package name="SOT223">
</package>
<package name="SOT143">
</package>
<package name="DB9_TE">
<description>TE Connectivity SUB-D male 9pin, right angle, 8.08mm 
1734351-1</description>
</package>
<package name="CORTEX_SWD_TH_2X5">
</package>
<package name="HSEC8-130-01-X-DV-A">
<description>0.8MM PITCH HIGH SPEED ASSEMBLY, 60PINS</description>
</package>
<package name="SOIC08">
</package>
<package name="FPC_REBEL_SFW6R-1ST">
<description>FCI FPC connector SFW6R-1STE1LF

according to Drawing JSA 96336 / revision D, Nov 1, 2009

used in Rebelsim FPC</description>
</package>
<package name="1X06">
<description>&lt;b&gt;PIN HEADER&lt;/b&gt;</description>
</package>
<package name="1X06/90">
<description>&lt;b&gt;PIN HEADER&lt;/b&gt;</description>
</package>
<package name="1X02">
<description>&lt;b&gt;PIN HEADER&lt;/b&gt;</description>
</package>
<package name="1X02/90">
<description>&lt;b&gt;PIN HEADER&lt;/b&gt;</description>
</package>
<package name="2X10">
<description>&lt;b&gt;PIN HEADER&lt;/b&gt;</description>
</package>
<package name="2X10/90">
<description>&lt;b&gt;PIN HEADER&lt;/b&gt;</description>
</package>
<package name="2X20">
<description>&lt;b&gt;PIN HEADER&lt;/b&gt;</description>
</package>
<package name="2X20/90">
<description>&lt;b&gt;PIN HEADER&lt;/b&gt;</description>
</package>
<package name="2X05">
<description>&lt;b&gt;PIN HEADER&lt;/b&gt;</description>
</package>
<package name="2X05/90">
<description>&lt;b&gt;PIN HEADER&lt;/b&gt;</description>
</package>
<package name="TSSOP16L">
<description>&lt;b&gt;MOLDED TSSOP&lt;/b&gt; JEDEC, 5 x 4.4 x 9.9 mm Body 16 LD, 0.65mm Pitch&lt;p&gt;
Source: http://www.national.com/packaging/mkt/mtc16.pdf</description>
</package>
<package name="1X08">
<description>&lt;b&gt;PIN HEADER&lt;/b&gt;</description>
</package>
<package name="1X08/90">
<description>&lt;b&gt;PIN HEADER&lt;/b&gt;</description>
</package>
<package name="DIP_SW_SMD-02">
<description>Omron A6S-210x-H</description>
</package>
<package name="WAVECOM_Q26">
</package>
<package name="P5K_100_SOCKET">
</package>
<package name="SSOP20">
</package>
<package name="L1210">
<description>INDUCTOR 1210</description>
</package>
<package name="TO252-3L">
<description>TO252-3L as per AP1084 data sheet</description>
</package>
<package name="1X3_SMD_90">
<description>From Sullins G_C__S__N-M89 data sheet Rev. D (11/12/2009)</description>
</package>
<package name="CTS_4SMD">
<description>CTS 4-SMD package taken from Doc. 008-0250-0 of CTS Electronic Components, Inc</description>
</package>
<package name="SUBD9M-SMD">
<description>NorComp 190-009-163R001</description>
</package>
<package name="1X02_SMD">
</package>
<package name="1X03_SMD">
</package>
<package name="NHD-C0216CIZ-FSW-FBW-3V3">
<description>Newhaven Display NHD-C0216CiZ-FSW-FBW-3V3</description>
</package>
<package name="DIP_SP6T">
</package>
<package name="4PDT_DIL12">
</package>
<package name="MOLEX_MICROSTACK_12PIN">
<description>Molex MicroStack 503548-1220</description>
</package>
<package name="FPC_SODLER_6">
</package>
<package name="AXE580124">
<description>Panasonic A4S Series, AXE580124 (socket)</description>
</package>
<package name="FPC_SOLDER_10">
</package>
<package name="FPC_SOLDER_20">
</package>
<package name="SFV20R-1ST">
<description>FCI SFV20R-1ST__HLF, 20pos 0.5mm pitch FPC slide connector, lower contact type</description>
</package>
<package name="TE184952-0">
</package>
<package name="RADITEK_4217">
</package>
<package name="1X2_SMD_90">
</package>
<package name="RGE_S_PVQFN_N24">
<description>Texas Instruments RGE (S-PVQFN-N24)</description>
</package>
<package name="MINISO8">
</package>
<package name="TY_NR_SERIES">
<description>Taio Yuden SMD Poewr Inductors (NR Series)

Footprint for (at least) NRS6010, NR 6012, NRS6012, NRS6014, NR6020, NRS6020, NR6028, NRS6028,  NR6045, NRS6045</description>
</package>
<package name="TSOP-6">
<description>TSOP-6 CAS E318G-02 ISSUE V (ON Semiconductor)</description>
</package>
<package name="SOT23L">
</package>
<package name="SOT666">
<description>SOT666 package outline (NXP semiconductors, taken from PED5V0U5BV DS 04-11-08)</description>
</package>
<package name="UFM">
<description>Toshiba UFM (2-2U1A)</description>
</package>
<package name="SSOP8">
<description>SSOP8 / TI DCT (R-PDSO-G8) 09/02</description>
</package>
<package name="2X05_SMD_90">
</package>
<package name="ELNA_DC_E">
</package>
<package name="MK16">
<description>MEDER electronic MK16 series</description>
</package>
<package name="USON6">
<description>ti R-PUSON-N6</description>
</package>
<package name="UC530M">
<description>u-blox UC530M Data Sheet FTX-HW-12007-A Figure 8 and Figure 7</description>
</package>
<package name="29228-5">
<description>AMP 292228-5 Mini CT Connector 1.5mm PITCH

SMD TYPE WITHOUT BOSS</description>
</package>
<package name="SF7W008S1A">
</package>
<package name="IFSC-1515AH">
<description>Vishay IFSC-1515AH-01</description>
</package>
<package name="SRN1060">
<description>Bourns SRN1060 Series semi-shielded power inductors</description>
</package>
<package name="CDRH4D28">
<description>Sumida CDRH4D28</description>
</package>
<package name="SOD323">
</package>
<package name="SOT89">
</package>
<package name="SRP1250">
<description>Bourns SRP1250</description>
</package>
<package name="USB_A_VERT">
<description>Amphenol UE27-AEX4-X0X</description>
</package>
<package name="USB_A_HORIZ">
<description>Würth Elektronik  614 004 160 21</description>
</package>
<package name="SOT23-6">
</package>
<package name="SMBJ">
</package>
<package name="USB-A-MALE">
<description>USB A male plug THT, Molex Drawing SD-48037-001</description>
</package>
<package name="LUM_KLB13">
<description>Lumberg KLB 13 2.5mm stereo jack, vertical</description>
</package>
<package name="VQFN-N16">
</package>
<package name="2X05/90-WUERTH">
</package>
<package name="ABRACON_ABM10">
<description>Abracon ABM10 Crystal Package</description>
</package>
<package name="ABM3">
<description>Abracon ABM3 crystal package</description>
</package>
<package name="BA2032-SM">
</package>
<package name="2X05_SMD_180">
<description>
</description>
</package>
<package name="2X08_SMD_180">
</package>
<package name="2X02_SMD_180">
</package>
<package name="2X03_SMD_180">
</package>
<package name="1X05_SMD">
</package>
<package name="DBV_SOT23-6">
<description>TI DBV (R-PDSO-G6) package (SOT23-6</description>
</package>
<package name="1X03">
</package>
<package name="1X03_LOCK">
</package>
<package name="1X03_LOCK_LONGPADS">
</package>
<package name="1X03_LOCK_NO_SILK">
</package>
<package name="2X03_SMD_180_SP">
</package>
<package name="SOT363">
<description>SC-88 or SOT363 or US6 or UMT6 or S-Mini6 or SC-70-6 &lt;p&gt;

https://www.nxp.com/docs/en/package-information/SOT363.pdf</description>
</package>
<package name="PULSE_BH">
</package>
</packages>
<symbols>
<symbol name="COAX-F-4GND">
<pin name="1" direction="pas"/>
<pin name="GND@3" direction="pwr"/>
<pin name="GND@4" direction="pwr"/>
<pin name="GND@2" direction="pwr"/>
<pin name="GND@1" direction="pwr"/>
</symbol>
<symbol name="COAX-M-2GND">
<description>&lt;b&gt;Coaxial connector - male&lt;/b&gt;&lt;br&gt;&lt;br&gt;
2 GND connections</description>
<pin name="1" direction="pas"/>
<pin name="GND@2" direction="pwr"/>
<pin name="GND@1" direction="pwr"/>
</symbol>
<symbol name="NCN8025">
<pin name="VDDP" direction="pwr"/>
<pin name="VSEL0" direction="in"/>
<pin name="VSEL1" direction="in"/>
<pin name="/CMDVCC" direction="in"/>
<pin name="/INT" direction="out"/>
<pin name="CLKDIV1" direction="in"/>
<pin name="CLKDIV2"/>
<pin name="CLKIN"/>
<pin name="RSTIN" direction="in"/>
<pin name="IO_UC"/>
<pin name="GND2" direction="pwr"/>
<pin name="C_RST" direction="out"/>
<pin name="C_IO"/>
<pin name="C_CLK" direction="out"/>
<pin name="/PRES" direction="in"/>
<pin name="C_VCC" direction="in"/>
<pin name="VDD" direction="pwr"/>
</symbol>
<symbol name="NC8025A">
<pin name="GND" direction="pwr"/>
<pin name="VDDP" direction="pwr"/>
<pin name="PORADJ" direction="in"/>
<pin name="VSEL0" direction="in"/>
<pin name="VSEL1" direction="in"/>
<pin name="/CMDVCC" direction="in"/>
<pin name="/INT" direction="out"/>
<pin name="CLKDIV1" direction="in"/>
<pin name="CLKDIV2"/>
<pin name="CLKIN"/>
<pin name="RSTIN" direction="in"/>
<pin name="IO_UC"/>
<pin name="AUX1_UC"/>
<pin name="AUX2_UC"/>
<pin name="GND2" direction="pwr"/>
<pin name="C_RST" direction="out"/>
<pin name="C_IO"/>
<pin name="C_AUX1"/>
<pin name="GND3"/>
<pin name="C_AUX2"/>
<pin name="C_CLK" direction="out"/>
<pin name="PRES" direction="in"/>
<pin name="/PRES" direction="in"/>
<pin name="C_VCC" direction="in"/>
<pin name="VDD" direction="pwr"/>
</symbol>
<symbol name="SIM">
<pin name="VCC" direction="pwr"/>
<pin name="RST" direction="in"/>
<pin name="CLK" direction="in"/>
<pin name="AUX1"/>
<pin name="AUX2"/>
<pin name="I/O"/>
<pin name="VPP" direction="pwr"/>
<pin name="GND"/>
</symbol>
<symbol name="SIM_SW_NO">
<pin name="0@A" direction="pas"/>
<pin name="1@A" direction="pas"/>
</symbol>
<symbol name="CON_CORTEX_DBG">
<pin name="VCC" direction="pwr"/>
<pin name="GND" direction="pwr"/>
<pin name="GND2" direction="pwr"/>
<pin name="KEY"/>
<pin name="GNDDETECT"/>
<pin name="/RESET"/>
<pin name="NC"/>
<pin name="SWO"/>
<pin name="SWDCLK"/>
<pin name="SWDIO"/>
</symbol>
<symbol name="IDT82V2081_TDM">
<pin name="LOS" direction="out"/>
<pin name="RCLK" direction="out"/>
<pin name="RD/RDP" direction="out"/>
<pin name="CV/RDN" direction="out"/>
<pin name="TCLK" direction="in"/>
<pin name="TD/TDP" direction="in"/>
<pin name="TDN" direction="in"/>
</symbol>
<symbol name="IDT82V2081_LINE">
<pin name="RTIP" direction="in"/>
<pin name="RRING" direction="in"/>
<pin name="TTIP" direction="out"/>
<pin name="TRING" direction="out"/>
</symbol>
<symbol name="IDT82V2081_SERIAL">
<pin name="!INT" direction="out"/>
<pin name="!CS" direction="in"/>
<pin name="SDO/!ACK/RDY" direction="out"/>
<pin name="SCLK/ALE/AS" direction="in"/>
<pin name="!RD/DS/SCLKE" direction="in"/>
<pin name="SDI/WR/RW" direction="in"/>
</symbol>
<symbol name="IDT82V2081_PINCTRL">
<pin name="MODE0" direction="in"/>
<pin name="MODE1" direction="in"/>
<pin name="PULS0/AD4" direction="in"/>
<pin name="PULS1/AD5" direction="in"/>
<pin name="PULS2/AD6" direction="in"/>
<pin name="PULS3/AD7" direction="in"/>
<pin name="EQ/AD3" direction="in"/>
<pin name="RPD/AD2" direction="in"/>
<pin name="PATT1/AD1" direction="in"/>
<pin name="PATT0/AD0" direction="in"/>
<pin name="JA0" direction="in"/>
<pin name="JA1" direction="in"/>
<pin name="THZ" direction="in"/>
<pin name="!RST" direction="in"/>
<pin name="RCLKE" direction="in"/>
</symbol>
<symbol name="IDT82V2081_V">
<pin name="GNDT" direction="pwr"/>
<pin name="GNDA" direction="pwr"/>
<pin name="VDDD" direction="pwr"/>
<pin name="VDDT" direction="pwr"/>
<pin name="REF" direction="in"/>
<pin name="GNDD" direction="pwr"/>
<pin name="VDDA" direction="pwr"/>
<pin name="VDDIO" direction="pwr"/>
<pin name="GNDIO" direction="pwr"/>
</symbol>
<symbol name="IDT82V2081_MISC">
<pin name="MCLK" direction="pwr"/>
<pin name="IC0" direction="nc"/>
<pin name="IC1" direction="nc"/>
</symbol>
<symbol name="OSCILLATOR">
<pin name="E/D" direction="in"/>
<pin name="VCC" direction="pwr"/>
<pin name="GND" direction="pwr"/>
<pin name="OUT" direction="out"/>
</symbol>
<symbol name="RESNET8">
<pin name="2" direction="pas"/>
<pin name="3" direction="pas"/>
<pin name="4" direction="pas"/>
<pin name="5" direction="pas"/>
<pin name="6" direction="pas"/>
<pin name="7" direction="pas"/>
<pin name="8" direction="pas"/>
<pin name="1" direction="pas"/>
<pin name="C" direction="pas"/>
<pin name="D" direction="pas"/>
</symbol>
<symbol name="NV08C-CSM">
<pin name="ANT_GND1"/>
<pin name="ANT_IN" direction="in"/>
<pin name="ANT_GND2"/>
<pin name="GPIO0"/>
<pin name="GPIO1"/>
<pin name="GPIO2"/>
<pin name="GPIO3"/>
<pin name="GPIO4"/>
<pin name="GPIO5"/>
<pin name="GPIO6"/>
<pin name="GPIO7"/>
<pin name="RX1" direction="in"/>
<pin name="TX1" direction="out"/>
<pin name="RX2" direction="in"/>
<pin name="TX2" direction="out"/>
<pin name="VIN_A" direction="pwr"/>
<pin name="RF_SHDN" direction="out"/>
<pin name="VBAT" direction="in"/>
<pin name="VIN_D" direction="pwr"/>
<pin name="VCCIO" direction="pwr"/>
<pin name="GND1"/>
<pin name="GND2"/>
<pin name="GND3"/>
<pin name="GND4"/>
<pin name="GND5"/>
<pin name="GND6"/>
<pin name="GND7"/>
<pin name="GND8"/>
<pin name="GND9"/>
<pin name="GND10"/>
<pin name="GND11"/>
<pin name="GND12"/>
<pin name="!RES" direction="in"/>
<pin name="GND13"/>
<pin name="GND14"/>
</symbol>
<symbol name="JACK2.5STEREO">
<pin name="RING" direction="pas"/>
<pin name="TIP" direction="pas"/>
<pin name="MIDDLE" direction="pas"/>
</symbol>
<symbol name="BATTERY">
<pin name="+" direction="pas"/>
<pin name="-" direction="pas"/>
<pin name="+@1" direction="pas"/>
</symbol>
<symbol name="COAX_FGND">
<pin name="1" direction="pas"/>
<pin name="GND" direction="pwr"/>
</symbol>
<symbol name="GND">
<pin name="GND" direction="pwr"/>
</symbol>
<symbol name="L-EU">
<pin name="2" direction="pas"/>
<pin name="1" direction="pas"/>
</symbol>
<symbol name="SP3203E">
<pin name="C1+"/>
<pin name="C1-"/>
<pin name="C2+"/>
<pin name="C2-"/>
<pin name="T1IN" direction="in"/>
<pin name="T2IN" direction="in"/>
<pin name="R1OUT" direction="out"/>
<pin name="R2OUT" direction="out"/>
<pin name="V+"/>
<pin name="V-"/>
<pin name="T1OUT" direction="out"/>
<pin name="T2OUT" direction="out"/>
<pin name="R1IN" direction="in"/>
<pin name="R2IN" direction="in"/>
<pin name="VL" direction="pwr"/>
<pin name="VCC" direction="pwr"/>
<pin name="!SHDN" direction="in"/>
<pin name="GND"/>
<pin name="T3IN" direction="in"/>
<pin name="T3OUT" direction="out"/>
</symbol>
<symbol name="74*2T45">
<pin name="1A"/>
<pin name="2A"/>
<pin name="2B"/>
<pin name="1B"/>
<pin name="DIR" direction="in"/>
<pin name="VCC_B" direction="pwr"/>
<pin name="VCC_A"/>
<pin name="GND" direction="pas"/>
</symbol>
<symbol name="74*4T245">
<pin name="1A1"/>
<pin name="1A2"/>
<pin name="1B2"/>
<pin name="1B1"/>
<pin name="1DIR" direction="in"/>
<pin name="VCC_B" direction="pwr"/>
<pin name="VCC_A"/>
<pin name="GND" direction="pas"/>
<pin name="2A1"/>
<pin name="2A2"/>
<pin name="2B2"/>
<pin name="2B1"/>
<pin name="2DIR" direction="in"/>
<pin name="GND1" direction="pas"/>
<pin name="!1OE" direction="in"/>
<pin name="!2OE" direction="in"/>
</symbol>
<symbol name="DIODE_ARRAY3">
<pin name="A" direction="pas"/>
<pin name="K" direction="pas"/>
<pin name="K1" direction="pas"/>
<pin name="K2" direction="pas"/>
</symbol>
<symbol name="SUBD9M">
<pin name="1" direction="pas"/>
<pin name="6" direction="pas"/>
<pin name="2" direction="pas"/>
<pin name="7" direction="pas"/>
<pin name="3" direction="pas"/>
<pin name="8" direction="pas"/>
<pin name="4" direction="pas"/>
<pin name="9" direction="pas"/>
<pin name="5" direction="pas"/>
<pin name="G1" direction="pas"/>
<pin name="G2" direction="pas"/>
</symbol>
<symbol name="SYSMOBTS_PROD_PWR">
<pin name="5VDC_1" direction="sup"/>
<pin name="5VDC_2" direction="sup"/>
<pin name="3V3DC_1" direction="sup"/>
<pin name="3V3DC_2" direction="sup"/>
<pin name="1V8DC_1" direction="sup"/>
<pin name="1V8DC_2" direction="sup"/>
<pin name="1V2DC_1" direction="sup"/>
<pin name="1V2DC_2" direction="sup"/>
<pin name="1V2CORE_1" direction="sup"/>
<pin name="1V2CORE_2" direction="sup"/>
<pin name="GND5" direction="sup"/>
<pin name="GND4" direction="sup"/>
<pin name="GND3" direction="sup"/>
<pin name="GND2" direction="sup"/>
<pin name="GND1" direction="sup"/>
</symbol>
<symbol name="SYSMOBTS_PROD_SPI">
<pin name="SPICLK" direction="out"/>
<pin name="SPIEN1" direction="out"/>
<pin name="SPIEN0" direction="out"/>
<pin name="SPIDI" direction="in"/>
<pin name="SPIDO" direction="out"/>
<pin name="GND1" direction="pas"/>
<pin name="GND2" direction="pas"/>
<pin name="DSP_BTSEL1" direction="in"/>
<pin name="DSP_BTSEL0" direction="in"/>
<pin name="UART_TX0" direction="out"/>
<pin name="UART_RX0" direction="in"/>
<pin name="I2C_SDA"/>
<pin name="I2C_SCL"/>
</symbol>
<symbol name="SYSMOBTS_PROD_FPGA_JTAG">
<pin name="FPGA_TDI" direction="in"/>
<pin name="FPGA_TDO" direction="out"/>
<pin name="FPGA_TCK" direction="in"/>
<pin name="FPGA_TMS" direction="in"/>
<pin name="FPGA_GND" direction="pas"/>
</symbol>
<symbol name="SYSMOBTS_PROD_DSP_JTAG">
<pin name="DSP_TMS" direction="in"/>
<pin name="DSP_TRST" direction="in"/>
<pin name="DSP_TDI" direction="in"/>
<pin name="DSP_TDO" direction="out"/>
<pin name="DSP_RTCK" direction="out"/>
<pin name="DSP_TCK" direction="in"/>
<pin name="DSP_EMU0" direction="sup"/>
<pin name="DSP_EMU1" direction="sup"/>
<pin name="DSP_GND" direction="sup"/>
</symbol>
<symbol name="SYSMOBTS_CPLD_JTAG">
<pin name="CPLD_TCK" direction="sup"/>
<pin name="CPLD_TDI" direction="sup"/>
<pin name="CPLD_TDO" direction="sup"/>
<pin name="CPLD_TMS" direction="sup"/>
<pin name="CPLD_GND" direction="sup"/>
</symbol>
<symbol name="IDT_ICS501">
<pin name="VCC" direction="pwr"/>
<pin name="S0" direction="in"/>
<pin name="S1" direction="in"/>
<pin name="GND" direction="pas"/>
<pin name="X1_ICLK" direction="in"/>
<pin name="X2" direction="out"/>
<pin name="CLK" direction="out"/>
<pin name="OE" direction="in"/>
</symbol>
<symbol name="REBELFPC_CON">
<pin name="VCC" direction="pwr" function="dot"/>
<pin name="!RST" direction="out" function="dot"/>
<pin name="CLK" direction="out" function="dot"/>
<pin name="I/O" function="dot"/>
<pin name="VPP" direction="pwr" function="dot"/>
<pin name="GND" direction="pas" function="dot"/>
</symbol>
<symbol name="PINHD2">
<pin name="1" direction="pas" function="dot"/>
<pin name="2" direction="pas" function="dot"/>
</symbol>
<symbol name="PINH2X10">
<pin name="1" direction="pas" function="dot"/>
<pin name="2" direction="pas" function="dot"/>
<pin name="3" direction="pas" function="dot"/>
<pin name="4" direction="pas" function="dot"/>
<pin name="5" direction="pas" function="dot"/>
<pin name="6" direction="pas" function="dot"/>
<pin name="7" direction="pas" function="dot"/>
<pin name="8" direction="pas" function="dot"/>
<pin name="9" direction="pas" function="dot"/>
<pin name="10" direction="pas" function="dot"/>
<pin name="11" direction="pas" function="dot"/>
<pin name="12" direction="pas" function="dot"/>
<pin name="13" direction="pas" function="dot"/>
<pin name="14" direction="pas" function="dot"/>
<pin name="15" direction="pas" function="dot"/>
<pin name="16" direction="pas" function="dot"/>
<pin name="17" direction="pas" function="dot"/>
<pin name="18" direction="pas" function="dot"/>
<pin name="19" direction="pas" function="dot"/>
<pin name="20" direction="pas" function="dot"/>
</symbol>
<symbol name="PINH2X20">
<pin name="1" direction="pas" function="dot"/>
<pin name="2" direction="pas" function="dot"/>
<pin name="3" direction="pas" function="dot"/>
<pin name="4" direction="pas" function="dot"/>
<pin name="5" direction="pas" function="dot"/>
<pin name="6" direction="pas" function="dot"/>
<pin name="7" direction="pas" function="dot"/>
<pin name="8" direction="pas" function="dot"/>
<pin name="9" direction="pas" function="dot"/>
<pin name="10" direction="pas" function="dot"/>
<pin name="11" direction="pas" function="dot"/>
<pin name="12" direction="pas" function="dot"/>
<pin name="13" direction="pas" function="dot"/>
<pin name="14" direction="pas" function="dot"/>
<pin name="15" direction="pas" function="dot"/>
<pin name="16" direction="pas" function="dot"/>
<pin name="17" direction="pas" function="dot"/>
<pin name="18" direction="pas" function="dot"/>
<pin name="19" direction="pas" function="dot"/>
<pin name="20" direction="pas" function="dot"/>
<pin name="21" direction="pas" function="dot"/>
<pin name="22" direction="pas" function="dot"/>
<pin name="23" direction="pas" function="dot"/>
<pin name="24" direction="pas" function="dot"/>
<pin name="25" direction="pas" function="dot"/>
<pin name="26" direction="pas" function="dot"/>
<pin name="27" direction="pas" function="dot"/>
<pin name="28" direction="pas" function="dot"/>
<pin name="29" direction="pas" function="dot"/>
<pin name="30" direction="pas" function="dot"/>
<pin name="31" direction="pas" function="dot"/>
<pin name="32" direction="pas" function="dot"/>
<pin name="33" direction="pas" function="dot"/>
<pin name="34" direction="pas" function="dot"/>
<pin name="35" direction="pas" function="dot"/>
<pin name="36" direction="pas" function="dot"/>
<pin name="37" direction="pas" function="dot"/>
<pin name="38" direction="pas" function="dot"/>
<pin name="39" direction="pas" function="dot"/>
<pin name="40" direction="pas" function="dot"/>
</symbol>
<symbol name="PINH2X5">
<pin name="1" direction="pas" function="dot"/>
<pin name="2" direction="pas" function="dot"/>
<pin name="3" direction="pas" function="dot"/>
<pin name="4" direction="pas" function="dot"/>
<pin name="5" direction="pas" function="dot"/>
<pin name="6" direction="pas" function="dot"/>
<pin name="7" direction="pas" function="dot"/>
<pin name="8" direction="pas" function="dot"/>
<pin name="9" direction="pas" function="dot"/>
<pin name="10" direction="pas" function="dot"/>
</symbol>
<symbol name="SC16IS740">
<pin name="VDD" direction="pwr"/>
<pin name="!RESET" direction="in"/>
<pin name="SCLK" direction="in"/>
<pin name="!CS" direction="in"/>
<pin name="SO" direction="out"/>
<pin name="SI" direction="in"/>
<pin name="!SPI" direction="in"/>
<pin name="TX" direction="out"/>
<pin name="RX" direction="in"/>
<pin name="!RTS" direction="out"/>
<pin name="!CTS" direction="in"/>
<pin name="XTAL1" direction="pas"/>
<pin name="XTAL2" direction="pas"/>
<pin name="VSS" direction="pas"/>
<pin name="!IRQ" direction="out"/>
<pin name="VSS2" direction="pas"/>
</symbol>
<symbol name="PINHD8">
<pin name="1" direction="pas" function="dot"/>
<pin name="2" direction="pas" function="dot"/>
<pin name="3" direction="pas" function="dot"/>
<pin name="4" direction="pas" function="dot"/>
<pin name="5" direction="pas" function="dot"/>
<pin name="6" direction="pas" function="dot"/>
<pin name="7" direction="pas" function="dot"/>
<pin name="8" direction="pas" function="dot"/>
</symbol>
<symbol name="SW_DIP-02">
<pin name="3" direction="pas"/>
<pin name="4" direction="pas"/>
<pin name="1" direction="pas"/>
<pin name="2" direction="pas"/>
</symbol>
<symbol name="WAVECOM_Q268X_PS">
<description>Wavecom Q268x Power Supply</description>
<pin name="VBATT1" direction="pwr"/>
<pin name="VBATT2" direction="pwr"/>
<pin name="VBATT3" direction="pwr"/>
<pin name="VBATT4" direction="pwr"/>
<pin name="CHG_IN1" direction="pwr"/>
<pin name="CHG_IN2" direction="pwr"/>
<pin name="BAT_RTC" direction="pwr"/>
<pin name="GND1" direction="pas"/>
<pin name="GND2"/>
<pin name="GND3"/>
<pin name="GND4"/>
</symbol>
<symbol name="WAVECOM_Q268X_SIM">
<pin name="SIMPRES" direction="in"/>
<pin name="SIM_VCC" direction="pwr"/>
<pin name="!SIM_RST" direction="out"/>
<pin name="SIM_CLK" direction="out"/>
<pin name="SIM_IO"/>
</symbol>
<symbol name="WAVECOM_Q268X_AUDIO">
<pin name="MIC1P" direction="pas"/>
<pin name="MIC1N" direction="pas"/>
<pin name="MIC2P" direction="pas"/>
<pin name="MIC2N"/>
<pin name="SPK1P" direction="out"/>
<pin name="SPK1N" direction="out"/>
<pin name="SPK2P" direction="out"/>
<pin name="SPK2N" direction="out"/>
</symbol>
<symbol name="WAVECOM_Q268X_RS232">
<pin name="RXD" direction="in"/>
<pin name="TXD" direction="out"/>
<pin name="!RTS" direction="in"/>
<pin name="!CTS" direction="out"/>
<pin name="!RI" direction="out"/>
<pin name="!DCD" direction="out"/>
<pin name="!DSR" direction="out"/>
<pin name="!DTR" direction="in"/>
<pin name="RXD2" direction="in"/>
<pin name="TXD2" direction="out"/>
<pin name="!CTS2" direction="out"/>
<pin name="!RTS2" direction="in"/>
</symbol>
<symbol name="WAVECOM_Q268X_PCM">
<description>Wavecom digital PCM audio interface</description>
<pin name="PCM_SYNC" direction="out"/>
<pin name="PCM_CLK" direction="out"/>
<pin name="PCM_IN" direction="in"/>
<pin name="PCM_OUT" direction="out"/>
</symbol>
<symbol name="WAVECOM_Q268X_USB">
<pin name="VPAD_USB" direction="pwr"/>
<pin name="USB_DP"/>
<pin name="USB_DN"/>
</symbol>
<symbol name="WAVECOM_Q268X_MISC">
<pin name="VCC_1V8" direction="pwr"/>
<pin name="VCC_2V8" direction="pwr"/>
<pin name="BUZZER" direction="out"/>
<pin name="LED0" direction="out"/>
<pin name="BOOT" direction="in"/>
<pin name="!RESET" direction="in"/>
<pin name="ON_!OFF" direction="in"/>
<pin name="ADC2" direction="in"/>
<pin name="BAT_TEMP" direction="in"/>
</symbol>
<symbol name="MAX3218">
<description>Maxim MAX3218 1.8V to 4.24V-powered RS232 transceiver</description>
<pin name="FORCEON" direction="in"/>
<pin name="!FORCEOFF" direction="in"/>
<pin name="T1IN" direction="in"/>
<pin name="T2IN" direction="in"/>
<pin name="!INVALID" direction="out"/>
<pin name="R1OUT" direction="out"/>
<pin name="R2OUT" direction="out"/>
<pin name="T1OUT" direction="out"/>
<pin name="T2OUT" direction="out"/>
<pin name="R1IN" direction="in"/>
<pin name="R2IN" direction="in"/>
<pin name="C1N" direction="pas"/>
<pin name="C1P" direction="pas"/>
<pin name="VN" direction="pas"/>
<pin name="VP" direction="pas"/>
<pin name="LX" direction="pas"/>
<pin name="VCC" direction="pas"/>
<pin name="GND" direction="pas"/>
<pin name="GND2" direction="pas"/>
<pin name="GND3" direction="pas"/>
</symbol>
<symbol name="WAVECOM_Q268X_SPI">
<description>Wavecom Q26 SPI / I2C / GPIO</description>
<pin name="SPI1_CLK" direction="out"/>
<pin name="SPI1_IO"/>
<pin name="SPI1_I" direction="in"/>
<pin name="SPI2_CLK" direction="out"/>
<pin name="SPI2_IO"/>
<pin name="SPI2_I" direction="in"/>
<pin name="I2C_SCL"/>
<pin name="I2C_SDA"/>
<pin name="GPIO0"/>
<pin name="GPIO1"/>
<pin name="GPIO2"/>
<pin name="GPIO19"/>
<pin name="GPIO20"/>
<pin name="GPIO21"/>
<pin name="GPIO22"/>
<pin name="GPIO23"/>
<pin name="GPIO3/INT0"/>
<pin name="GPIO25/INT1"/>
<pin name="GPIO24"/>
<pin name="GPIO31"/>
<pin name="GPIO35"/>
</symbol>
<symbol name="ESD_TVS_DIODE">
<pin name="A" direction="pas"/>
<pin name="K" direction="pas"/>
</symbol>
<symbol name="PINHD3">
<pin name="1" direction="pas" function="dot"/>
<pin name="2" direction="pas" function="dot"/>
<pin name="3" direction="pas" function="dot"/>
</symbol>
<symbol name="MAX3322E">
<pin name="RENABLE" direction="in"/>
<pin name="TXENABLE" direction="in"/>
<pin name="T1IN" direction="in"/>
<pin name="T2IN" direction="in"/>
<pin name="VL" direction="pwr"/>
<pin name="R1OUT" direction="out"/>
<pin name="R2OUT" direction="out"/>
<pin name="T1OUT" direction="out"/>
<pin name="T2OUT" direction="out"/>
<pin name="R1IN" direction="in"/>
<pin name="R2IN" direction="in"/>
<pin name="C1N" direction="pas"/>
<pin name="C1P" direction="pas"/>
<pin name="VN" direction="pas"/>
<pin name="VP" direction="pas"/>
<pin name="VCC" direction="pwr"/>
<pin name="!SHDN" direction="in"/>
<pin name="GND" direction="pas"/>
<pin name="C2N" direction="pas"/>
<pin name="C2P" direction="pas"/>
</symbol>
<symbol name="QG1">
<pin name="GND" direction="pwr"/>
<pin name="VCC" direction="pwr"/>
<pin name="FO" direction="out"/>
<pin name="OE" direction="in"/>
</symbol>
<symbol name="LCD">
<pin name="LED+" direction="pwr"/>
<pin name="LED-" direction="pas"/>
<pin name="VDD" direction="out"/>
<pin name="GND" direction="pas"/>
<pin name="VOUT" direction="pwr"/>
<pin name="C+" direction="pas"/>
<pin name="C-" direction="pas"/>
<pin name="!RST" direction="in"/>
<pin name="SDA"/>
<pin name="SCL"/>
</symbol>
<symbol name="SP6T">
<pin name="3"/>
<pin name="4"/>
<pin name="5"/>
<pin name="2"/>
<pin name="1"/>
<pin name="6"/>
<pin name="C"/>
</symbol>
<symbol name="SW_4PDT">
<pin name="A"/>
<pin name="A1"/>
<pin name="A2"/>
<pin name="B1"/>
<pin name="B2"/>
<pin name="B"/>
<pin name="C"/>
<pin name="C1"/>
<pin name="C2"/>
<pin name="D"/>
<pin name="D1"/>
<pin name="D2"/>
</symbol>
<symbol name="PINH2X6">
<pin name="1" direction="pas" function="dot"/>
<pin name="2" direction="pas" function="dot"/>
<pin name="3" direction="pas" function="dot"/>
<pin name="4" direction="pas" function="dot"/>
<pin name="5" direction="pas" function="dot"/>
<pin name="6" direction="pas" function="dot"/>
<pin name="7" direction="pas" function="dot"/>
<pin name="8" direction="pas" function="dot"/>
<pin name="9" direction="pas" function="dot"/>
<pin name="10" direction="pas" function="dot"/>
<pin name="11" direction="pas" function="dot"/>
<pin name="12" direction="pas" function="dot"/>
</symbol>
<symbol name="PINHD6">
<pin name="1" direction="pas" function="dot"/>
<pin name="2" direction="pas" function="dot"/>
<pin name="3" direction="pas" function="dot"/>
<pin name="4" direction="pas" function="dot"/>
<pin name="5" direction="pas" function="dot"/>
<pin name="6" direction="pas" function="dot"/>
</symbol>
<symbol name="I4S_DEBUG">
<description>Debug Connector as found on iPhone 4s beneath the SIM card slot</description>
<pin name="BATT_VCC2"/>
<pin name="BATT_VCC4"/>
<pin name="BATT_VCC6"/>
<pin name="BATT_VCC8"/>
<pin name="!DEBUG_RST_N"/>
<pin name="!RESET_PMU_N"/>
<pin name="!RADIO_ON_N"/>
<pin name="GND16"/>
<pin name="BB_USB_VBUS"/>
<pin name="BB_USB_DP"/>
<pin name="BB_USB_DN"/>
<pin name="GND24"/>
<pin name="BB_JTAG_TCK"/>
<pin name="BB_JTAG_TMS"/>
<pin name="BB_JTAG_TDO"/>
<pin name="BB_JTAG_TDI"/>
<pin name="!BB_JTAG_TRST_N"/>
<pin name="BB_JTAG_RTCK"/>
<pin name="GND38"/>
<pin name="GND62"/>
<pin name="BB_UART_TXD"/>
<pin name="BB_UART_RXD"/>
<pin name="!BB_UART_RTS_N"/>
<pin name="!BB_UART_CTS_N"/>
<pin name="DEBUG_GPIO_LED"/>
<pin name="BB_EMERGENCY_DWLD"/>
<pin name="FET_ON"/>
<pin name="SIMCRD_IO_CONN"/>
<pin name="SIMCRD_CLK_CONN"/>
<pin name="SIMCRD_RST_CONN"/>
<pin name="SIM_DETECT"/>
<pin name="VSIM_VAR"/>
<pin name="GND69"/>
<pin name="WLAN_SDIO_DATA0"/>
<pin name="WLAN_SDIO_DATA1"/>
<pin name="WLAN_SDIO_DATA2"/>
<pin name="WLAN_SDIO_DATA3"/>
<pin name="WLAN_SDIO_CMD"/>
<pin name="WLAN_SDIO_CLK"/>
<pin name="GND55"/>
<pin name="GND27"/>
<pin name="!BT_UART_CTS_N"/>
<pin name="!BT_UART_RTS_N"/>
<pin name="BT_UART_RXD"/>
<pin name="BT_UART_TXD"/>
<pin name="WLAN_REG_ON"/>
<pin name="!BT_RESET_N"/>
<pin name="GND13"/>
<pin name="!RF_RESET_N"/>
<pin name="VREG_MSME"/>
<pin name="BATT_VCC7"/>
<pin name="BATT_VCC3"/>
<pin name="BATT_VCC5"/>
<pin name="BATT_VCC1"/>
</symbol>
<symbol name="PINHD10">
<pin name="1" direction="pas" function="dot"/>
<pin name="2" direction="pas" function="dot"/>
<pin name="3" direction="pas" function="dot"/>
<pin name="4" direction="pas" function="dot"/>
<pin name="5" direction="pas" function="dot"/>
<pin name="6" direction="pas" function="dot"/>
<pin name="7" direction="pas" function="dot"/>
<pin name="8" direction="pas" function="dot"/>
<pin name="9" direction="pas" function="dot"/>
<pin name="10" direction="pas" function="dot"/>
</symbol>
<symbol name="PINHD20">
<pin name="1" direction="pas" function="dot"/>
<pin name="2" direction="pas" function="dot"/>
<pin name="3" direction="pas" function="dot"/>
<pin name="4" direction="pas" function="dot"/>
<pin name="5" direction="pas" function="dot"/>
<pin name="6" direction="pas" function="dot"/>
<pin name="7" direction="pas" function="dot"/>
<pin name="8" direction="pas" function="dot"/>
<pin name="9" direction="pas" function="dot"/>
<pin name="10" direction="pas" function="dot"/>
<pin name="11" direction="pas" function="dot"/>
<pin name="12" direction="pas" function="dot"/>
<pin name="13" direction="pas" function="dot"/>
<pin name="14" direction="pas" function="dot"/>
<pin name="15" direction="pas" function="dot"/>
<pin name="16" direction="pas" function="dot"/>
<pin name="17" direction="pas" function="dot"/>
<pin name="18" direction="pas" function="dot"/>
<pin name="19" direction="pas" function="dot"/>
<pin name="20" direction="pas" function="dot"/>
</symbol>
<symbol name="CER_DUP">
<pin name="COM"/>
<pin name="HI"/>
<pin name="LO"/>
</symbol>
<symbol name="RDUP_4217_GND">
<pin name="P$1"/>
<pin name="P$2"/>
<pin name="P$3"/>
<pin name="P$4"/>
<pin name="P$5"/>
<pin name="P$6"/>
<pin name="P$7"/>
</symbol>
<symbol name="STC3100">
<pin name="ROSC" direction="pas"/>
<pin name="IO0"/>
<pin name="SDA"/>
<pin name="SCL" direction="in"/>
<pin name="GND"/>
<pin name="CG"/>
<pin name="VCC"/>
<pin name="VIN" direction="pas"/>
</symbol>
<symbol name="BQ2416X">
<pin name="IN"/>
<pin name="USB"/>
<pin name="CD"/>
<pin name="SDA"/>
<pin name="SCL"/>
<pin name="DP"/>
<pin name="DN"/>
<pin name="STAT"/>
<pin name="INT"/>
<pin name="PMIDU"/>
<pin name="PMIDI"/>
<pin name="DRV"/>
<pin name="BOOT"/>
<pin name="SW"/>
<pin name="PGND"/>
<pin name="SYS"/>
<pin name="BAT"/>
<pin name="BGATE"/>
<pin name="TS"/>
</symbol>
<symbol name="NCP380">
<pin name="IN" direction="pas"/>
<pin name="!FLAG" direction="in"/>
<pin name="EN" direction="in"/>
<pin name="OUT" direction="pwr"/>
<pin name="ILIM" direction="pas"/>
<pin name="GND" direction="pas"/>
</symbol>
<symbol name="USB_TVS">
<pin name="1A" direction="pas"/>
<pin name="2A" direction="pas"/>
<pin name="2B" direction="pas"/>
<pin name="1B" direction="pas"/>
<pin name="VCC" direction="pas"/>
<pin name="GND" direction="pas"/>
</symbol>
<symbol name="TVS_5_BIDIR">
<pin name="1" direction="pas"/>
<pin name="2" direction="pas"/>
<pin name="5" direction="pas"/>
<pin name="4" direction="pas"/>
<pin name="3" direction="pas"/>
<pin name="GND" direction="pas"/>
</symbol>
<symbol name="P_MOSFET">
<pin name="S" direction="pas"/>
<pin name="G" direction="pas"/>
<pin name="D" direction="pas"/>
</symbol>
<symbol name="MONO_MULTIVIB">
<pin name="A" direction="in" function="dot"/>
<pin name="B" direction="in"/>
<pin name="CLR" direction="in" function="dot"/>
<pin name="GND" direction="pas"/>
<pin name="Q" direction="out"/>
<pin name="C" direction="in"/>
<pin name="R/C" direction="in"/>
<pin name="VCC" direction="pas"/>
</symbol>
<symbol name="UEXT">
<pin name="3V3" direction="pas" function="dot"/>
<pin name="GND" direction="pas" function="dot"/>
<pin name="TXD" direction="pas" function="dot"/>
<pin name="RXD" direction="pas" function="dot"/>
<pin name="SCL" direction="pas" function="dot"/>
<pin name="SDA" direction="pas" function="dot"/>
<pin name="MISO" direction="pas" function="dot"/>
<pin name="MOSI" direction="pas" function="dot"/>
<pin name="SCK" direction="pas" function="dot"/>
<pin name="SSEL" direction="pas" function="dot"/>
</symbol>
<symbol name="BATTERY2">
<pin name="-" direction="pas"/>
<pin name="+" direction="pas"/>
</symbol>
<symbol name="REED_SWITCH">
<pin name="1" direction="pas"/>
<pin name="2" direction="pas"/>
</symbol>
<symbol name="TPS389X">
<pin name="VCC" direction="pas"/>
<pin name="SENSE"/>
<pin name="GND" direction="pas"/>
<pin name="CT" direction="pas"/>
<pin name="EN" direction="in"/>
<pin name="OUT" direction="out"/>
</symbol>
<symbol name="YSEMI_BAT_PROT">
<pin name="VM"/>
<pin name="VT"/>
<pin name="GND"/>
<pin name="VDD"/>
</symbol>
<symbol name="UC530M">
<pin name="GND"/>
<pin name="TX0" direction="out"/>
<pin name="RX0" direction="in"/>
<pin name="TX1" direction="out"/>
<pin name="RX1" direction="in"/>
<pin name="!RESET" direction="in"/>
<pin name="UI_FIX" direction="out"/>
<pin name="FORCE_ON" direction="in"/>
<pin name="ANT" direction="out"/>
<pin name="RF_IN" direction="in"/>
<pin name="32K_DR_INT"/>
<pin name="EINT1"/>
<pin name="GPIO10"/>
<pin name="PPS" direction="out"/>
<pin name="WAKEUP"/>
<pin name="GPIO9"/>
<pin name="VDD" direction="pas"/>
<pin name="VDD_B" direction="pas"/>
</symbol>
<symbol name="74*125">
<pin name="OE" direction="in"/>
<pin name="I" direction="in"/>
<pin name="O" direction="hiz"/>
</symbol>
<symbol name="PWRN">
<pin name="GND" direction="pwr"/>
<pin name="VCC" direction="pwr"/>
</symbol>
<symbol name="PINHD5">
<pin name="1" direction="pas" function="dot"/>
<pin name="2" direction="pas" function="dot"/>
<pin name="3" direction="pas" function="dot"/>
<pin name="4" direction="pas" function="dot"/>
<pin name="5" direction="pas" function="dot"/>
</symbol>
<symbol name="D-ZENER">
<pin name="A" direction="pas"/>
<pin name="C" direction="pas"/>
</symbol>
<symbol name="USB-A">
<pin name="VBUS" direction="pas"/>
<pin name="D_N"/>
<pin name="D_P"/>
<pin name="GND" direction="pas"/>
<pin name="SHIELD" direction="pas"/>
</symbol>
<symbol name="MOSFET-N">
<pin name="G"/>
<pin name="S"/>
<pin name="D"/>
</symbol>
<symbol name="SUPPRESSOR">
<pin name="A" direction="pas"/>
<pin name="C" direction="pas"/>
</symbol>
<symbol name="TRS3232E">
<pin name="T1IN" direction="in"/>
<pin name="T2IN" direction="in"/>
<pin name="R1OUT" direction="out"/>
<pin name="R2OUT" direction="out"/>
<pin name="T1OUT" direction="out"/>
<pin name="T2OUT" direction="out"/>
<pin name="R1IN" direction="in"/>
<pin name="R2IN" direction="in"/>
<pin name="C1N" direction="pas"/>
<pin name="C1P" direction="pas"/>
<pin name="VN" direction="pas"/>
<pin name="VP" direction="pas"/>
<pin name="VCC" direction="pwr"/>
<pin name="GND" direction="pas"/>
<pin name="C2N" direction="pas"/>
<pin name="C2P" direction="pas"/>
</symbol>
<symbol name="Q-SHIELD">
<pin name="2" direction="pas"/>
<pin name="1" direction="pas"/>
<pin name="GND2" direction="pas"/>
<pin name="GND1" direction="pas"/>
</symbol>
<symbol name="Q">
<pin name="2" direction="pas"/>
<pin name="1" direction="pas"/>
</symbol>
<symbol name="PINH2X8">
<pin name="1" direction="pas" function="dot"/>
<pin name="2" direction="pas" function="dot"/>
<pin name="3" direction="pas" function="dot"/>
<pin name="4" direction="pas" function="dot"/>
<pin name="5" direction="pas" function="dot"/>
<pin name="6" direction="pas" function="dot"/>
<pin name="7" direction="pas" function="dot"/>
<pin name="8" direction="pas" function="dot"/>
<pin name="9" direction="pas" function="dot"/>
<pin name="10" direction="pas" function="dot"/>
<pin name="11" direction="pas" function="dot"/>
<pin name="12" direction="pas" function="dot"/>
<pin name="13" direction="pas" function="dot"/>
<pin name="14" direction="pas" function="dot"/>
<pin name="15" direction="pas" function="dot"/>
<pin name="16" direction="pas" function="dot"/>
</symbol>
<symbol name="PINH2X2">
<pin name="1" direction="pas" function="dot"/>
<pin name="2" direction="pas" function="dot"/>
<pin name="3" direction="pas" function="dot"/>
<pin name="4" direction="pas" function="dot"/>
</symbol>
<symbol name="PINH2X3">
<pin name="1" direction="pas" function="dot"/>
<pin name="2" direction="pas" function="dot"/>
<pin name="3" direction="pas" function="dot"/>
<pin name="4" direction="pas" function="dot"/>
<pin name="5" direction="pas" function="dot"/>
<pin name="6" direction="pas" function="dot"/>
</symbol>
<symbol name="74*1T45">
<pin name="1A"/>
<pin name="1B"/>
<pin name="DIR" direction="in"/>
<pin name="VCC_B" direction="pwr"/>
<pin name="VCC_A" direction="pwr"/>
<pin name="GND" direction="pwr"/>
</symbol>
<symbol name="M03">
<pin name="1" direction="pas"/>
<pin name="2" direction="pas"/>
<pin name="3" direction="pas"/>
</symbol>
<symbol name="74*126">
<pin name="OE" direction="in"/>
<pin name="I" direction="in"/>
<pin name="O" direction="hiz"/>
</symbol>
<symbol name="E1_MAGNETICS">
<pin name="P$1"/>
<pin name="P$2"/>
<pin name="P$3"/>
<pin name="P$4"/>
<pin name="P$5"/>
<pin name="P$6"/>
</symbol>
</symbols>
<devicesets>
<deviceset name="HRS_UFL" prefix="X" uservalue="yes">
<description>&lt;b&gt;Hirose U.FL SMT&lt;/b&gt;</description>
<gates>
<gate name="G$1" symbol="COAX-M-2GND"/>
</gates>
<devices>
<device name="" package="HRS_UFL">
<connects>
<connect gate="G$1" pin="1" pad="SIG"/>
<connect gate="G$1" pin="GND@1" pad="GND@1"/>
<connect gate="G$1" pin="GND@2" pad="GND@2"/>
</connects>
<technologies>
<technology name="">
<attribute name="OC_DIGIKEY" value="H9161CT-ND"/>
</technology>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="NCN8025">
<gates>
<gate name="G$1" symbol="NCN8025"/>
</gates>
<devices>
<device name="QFN16" package="QFN16_3X3">
<connects>
<connect gate="G$1" pin="/CMDVCC" pad="8"/>
<connect gate="G$1" pin="/INT" pad="11"/>
<connect gate="G$1" pin="/PRES" pad="3"/>
<connect gate="G$1" pin="CLKDIV1" pad="14"/>
<connect gate="G$1" pin="CLKDIV2" pad="15"/>
<connect gate="G$1" pin="CLKIN" pad="12"/>
<connect gate="G$1" pin="C_CLK" pad="5"/>
<connect gate="G$1" pin="C_IO" pad="4"/>
<connect gate="G$1" pin="C_RST" pad="6"/>
<connect gate="G$1" pin="C_VCC" pad="7"/>
<connect gate="G$1" pin="GND2" pad="EXP"/>
<connect gate="G$1" pin="IO_UC" pad="13"/>
<connect gate="G$1" pin="RSTIN" pad="9"/>
<connect gate="G$1" pin="VDD" pad="10"/>
<connect gate="G$1" pin="VDDP" pad="2"/>
<connect gate="G$1" pin="VSEL0" pad="1"/>
<connect gate="G$1" pin="VSEL1" pad="16"/>
</connects>
<technologies>
<technology name="">
<attribute name="OC_DIGIKEY" value="NCN8025MTTBGOSCT-ND"/>
</technology>
</technologies>
</device>
<device name="QFN24" package="QFN24_4X4">
<connects>
<connect gate="G$1" pin="/CMDVCC" pad="12"/>
<connect gate="G$1" pin="/INT" pad="17"/>
<connect gate="G$1" pin="/PRES" pad="3"/>
<connect gate="G$1" pin="CLKDIV1" pad="22"/>
<connect gate="G$1" pin="CLKDIV2" pad="23"/>
<connect gate="G$1" pin="CLKIN" pad="18"/>
<connect gate="G$1" pin="C_CLK" pad="9"/>
<connect gate="G$1" pin="C_IO" pad="5"/>
<connect gate="G$1" pin="C_RST" pad="10"/>
<connect gate="G$1" pin="C_VCC" pad="11"/>
<connect gate="G$1" pin="GND2" pad="25"/>
<connect gate="G$1" pin="IO_UC" pad="19"/>
<connect gate="G$1" pin="RSTIN" pad="14"/>
<connect gate="G$1" pin="VDD" pad="15"/>
<connect gate="G$1" pin="VDDP" pad="2"/>
<connect gate="G$1" pin="VSEL0" pad="1"/>
<connect gate="G$1" pin="VSEL1" pad="24"/>
</connects>
<technologies>
<technology name="">
<attribute name="OC_DIGIKEY" value="NCN8025AMNTXGOSCT-ND"/>
</technology>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="AMPHENOL_SIM" prefix="SIM">
<gates>
<gate name="-CARD" symbol="SIM"/>
<gate name="-DETECT" symbol="SIM_SW_NO"/>
</gates>
<devices>
<device name="" package="AMPHENOL_SIM">
<connects>
<connect gate="-CARD" pin="AUX1" pad="C7"/>
<connect gate="-CARD" pin="AUX2" pad="C8"/>
<connect gate="-CARD" pin="CLK" pad="CLK"/>
<connect gate="-CARD" pin="GND" pad="GND"/>
<connect gate="-CARD" pin="I/O" pad="IO"/>
<connect gate="-CARD" pin="RST" pad="RST"/>
<connect gate="-CARD" pin="VCC" pad="VCC_SIM"/>
<connect gate="-CARD" pin="VPP" pad="VPP"/>
<connect gate="-DETECT" pin="0@A" pad="SW1"/>
<connect gate="-DETECT" pin="1@A" pad="SW2"/>
</connects>
<technologies>
<technology name="">
<attribute name="OC_DIGIKEY" value="101-00271-82-1-ND "/>
</technology>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="CON_CORTEX_DBG">
<description>Connectors for the ARM CORTEX SWD</description>
<gates>
<gate name="G$1" symbol="CON_CORTEX_DBG"/>
</gates>
<devices>
<device name="" package="FTSH-105-01-XXX-DV-K">
<connects>
<connect gate="G$1" pin="/RESET" pad="10"/>
<connect gate="G$1" pin="GND" pad="3"/>
<connect gate="G$1" pin="GND2" pad="5"/>
<connect gate="G$1" pin="GNDDETECT" pad="9"/>
<connect gate="G$1" pin="KEY" pad="7"/>
<connect gate="G$1" pin="NC" pad="8"/>
<connect gate="G$1" pin="SWDCLK" pad="4"/>
<connect gate="G$1" pin="SWDIO" pad="2"/>
<connect gate="G$1" pin="SWO" pad="6"/>
<connect gate="G$1" pin="VCC" pad="1"/>
</connects>
<technologies>
<technology name=""/>
</technologies>
</device>
<device name="TH" package="CORTEX_SWD_TH_2X5">
<connects>
<connect gate="G$1" pin="/RESET" pad="10"/>
<connect gate="G$1" pin="GND" pad="3"/>
<connect gate="G$1" pin="GND2" pad="5"/>
<connect gate="G$1" pin="GNDDETECT" pad="9"/>
<connect gate="G$1" pin="KEY" pad="7"/>
<connect gate="G$1" pin="NC" pad="8"/>
<connect gate="G$1" pin="SWDCLK" pad="4"/>
<connect gate="G$1" pin="SWDIO" pad="2"/>
<connect gate="G$1" pin="SWO" pad="6"/>
<connect gate="G$1" pin="VCC" pad="1"/>
</connects>
<technologies>
<technology name=""/>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="IDT82V2081">
<gates>
<gate name="G$1" symbol="IDT82V2081_TDM"/>
<gate name="G$2" symbol="IDT82V2081_LINE"/>
<gate name="G$3" symbol="IDT82V2081_SERIAL"/>
<gate name="G$4" symbol="IDT82V2081_PINCTRL"/>
<gate name="G$5" symbol="IDT82V2081_V"/>
<gate name="G$6" symbol="IDT82V2081_MISC"/>
</gates>
<devices>
<device name="" package="TQFP44">
<connects>
<connect gate="G$1" pin="CV/RDN" pad="6"/>
<connect gate="G$1" pin="LOS" pad="7"/>
<connect gate="G$1" pin="RCLK" pad="4"/>
<connect gate="G$1" pin="RD/RDP" pad="5"/>
<connect gate="G$1" pin="TCLK" pad="1"/>
<connect gate="G$1" pin="TD/TDP" pad="2"/>
<connect gate="G$1" pin="TDN" pad="3"/>
<connect gate="G$2" pin="RRING" pad="40"/>
<connect gate="G$2" pin="RTIP" pad="41"/>
<connect gate="G$2" pin="TRING" pad="36"/>
<connect gate="G$2" pin="TTIP" pad="37"/>
<connect gate="G$3" pin="!CS" pad="21"/>
<connect gate="G$3" pin="!INT" pad="20"/>
<connect gate="G$3" pin="!RD/DS/SCLKE" pad="22"/>
<connect gate="G$3" pin="SCLK/ALE/AS" pad="25"/>
<connect gate="G$3" pin="SDI/WR/RW" pad="24"/>
<connect gate="G$3" pin="SDO/!ACK/RDY" pad="23"/>
<connect gate="G$4" pin="!RST" pad="12"/>
<connect gate="G$4" pin="EQ/AD3" pad="29"/>
<connect gate="G$4" pin="JA0" pad="14"/>
<connect gate="G$4" pin="JA1" pad="15"/>
<connect gate="G$4" pin="MODE0" pad="16"/>
<connect gate="G$4" pin="MODE1" pad="17"/>
<connect gate="G$4" pin="PATT0/AD0" pad="26"/>
<connect gate="G$4" pin="PATT1/AD1" pad="27"/>
<connect gate="G$4" pin="PULS0/AD4" pad="30"/>
<connect gate="G$4" pin="PULS1/AD5" pad="31"/>
<connect gate="G$4" pin="PULS2/AD6" pad="32"/>
<connect gate="G$4" pin="PULS3/AD7" pad="33"/>
<connect gate="G$4" pin="RCLKE" pad="11"/>
<connect gate="G$4" pin="RPD/AD2" pad="28"/>
<connect gate="G$4" pin="THZ" pad="13"/>
<connect gate="G$5" pin="GNDA" pad="39"/>
<connect gate="G$5" pin="GNDD" pad="10"/>
<connect gate="G$5" pin="GNDIO" pad="18"/>
<connect gate="G$5" pin="GNDT" pad="38"/>
<connect gate="G$5" pin="REF" pad="43"/>
<connect gate="G$5" pin="VDDA" pad="42"/>
<connect gate="G$5" pin="VDDD" pad="8"/>
<connect gate="G$5" pin="VDDIO" pad="19"/>
<connect gate="G$5" pin="VDDT" pad="35"/>
<connect gate="G$6" pin="IC0" pad="44"/>
<connect gate="G$6" pin="IC1" pad="34"/>
<connect gate="G$6" pin="MCLK" pad="9"/>
</connects>
<technologies>
<technology name="">
<attribute name="OC_DIGIKEY" value="800-2347-ND"/>
</technology>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="FOX_FXO-HC73">
<gates>
<gate name="G$1" symbol="OSCILLATOR"/>
</gates>
<devices>
<device name="" package="HC73">
<connects>
<connect gate="G$1" pin="E/D" pad="P$1"/>
<connect gate="G$1" pin="GND" pad="P$2"/>
<connect gate="G$1" pin="OUT" pad="P$3"/>
<connect gate="G$1" pin="VCC" pad="P$4"/>
</connects>
<technologies>
<technology name=""/>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="MNR">
<description>Rohm 8-element Chip Resistor Network

MNR35 (1206x5 size)</description>
<gates>
<gate name="G$1" symbol="RESNET8"/>
</gates>
<devices>
<device name="" package="MNR35">
<connects>
<connect gate="G$1" pin="1" pad="1"/>
<connect gate="G$1" pin="2" pad="2"/>
<connect gate="G$1" pin="3" pad="3"/>
<connect gate="G$1" pin="4" pad="4"/>
<connect gate="G$1" pin="5" pad="9"/>
<connect gate="G$1" pin="6" pad="8"/>
<connect gate="G$1" pin="7" pad="7"/>
<connect gate="G$1" pin="8" pad="6"/>
<connect gate="G$1" pin="C" pad="5"/>
<connect gate="G$1" pin="D" pad="10"/>
</connects>
<technologies>
<technology name=""/>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="NCN8025A">
<gates>
<gate name="G$1" symbol="NC8025A"/>
</gates>
<devices>
<device name="" package="QFN24_4X4">
<connects>
<connect gate="G$1" pin="/CMDVCC" pad="12"/>
<connect gate="G$1" pin="/INT" pad="17"/>
<connect gate="G$1" pin="/PRES" pad="3"/>
<connect gate="G$1" pin="AUX1_UC" pad="20"/>
<connect gate="G$1" pin="AUX2_UC" pad="21"/>
<connect gate="G$1" pin="CLKDIV1" pad="22"/>
<connect gate="G$1" pin="CLKDIV2" pad="23"/>
<connect gate="G$1" pin="CLKIN" pad="18"/>
<connect gate="G$1" pin="C_AUX1" pad="7"/>
<connect gate="G$1" pin="C_AUX2" pad="6"/>
<connect gate="G$1" pin="C_CLK" pad="9"/>
<connect gate="G$1" pin="C_IO" pad="5"/>
<connect gate="G$1" pin="C_RST" pad="10"/>
<connect gate="G$1" pin="C_VCC" pad="11"/>
<connect gate="G$1" pin="GND" pad="8"/>
<connect gate="G$1" pin="GND2" pad="16"/>
<connect gate="G$1" pin="GND3" pad="25"/>
<connect gate="G$1" pin="IO_UC" pad="19"/>
<connect gate="G$1" pin="PORADJ" pad="13"/>
<connect gate="G$1" pin="PRES" pad="4"/>
<connect gate="G$1" pin="RSTIN" pad="14"/>
<connect gate="G$1" pin="VDD" pad="15"/>
<connect gate="G$1" pin="VDDP" pad="2"/>
<connect gate="G$1" pin="VSEL0" pad="1"/>
<connect gate="G$1" pin="VSEL1" pad="24"/>
</connects>
<technologies>
<technology name=""/>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="NV08C-CSM">
<gates>
<gate name="G$1" symbol="NV08C-CSM"/>
</gates>
<devices>
<device name="" package="NV08C-CSM">
<connects>
<connect gate="G$1" pin="!RES" pad="25"/>
<connect gate="G$1" pin="ANT_GND1" pad="14"/>
<connect gate="G$1" pin="ANT_GND2" pad="16"/>
<connect gate="G$1" pin="ANT_IN" pad="15"/>
<connect gate="G$1" pin="GND1" pad="3"/>
<connect gate="G$1" pin="GND10" pad="22"/>
<connect gate="G$1" pin="GND11" pad="24"/>
<connect gate="G$1" pin="GND12" pad="27"/>
<connect gate="G$1" pin="GND13" pad="29"/>
<connect gate="G$1" pin="GND14" pad="34"/>
<connect gate="G$1" pin="GND2" pad="9"/>
<connect gate="G$1" pin="GND3" pad="10"/>
<connect gate="G$1" pin="GND4" pad="11"/>
<connect gate="G$1" pin="GND5" pad="12"/>
<connect gate="G$1" pin="GND6" pad="13"/>
<connect gate="G$1" pin="GND7" pad="17"/>
<connect gate="G$1" pin="GND8" pad="18"/>
<connect gate="G$1" pin="GND9" pad="19"/>
<connect gate="G$1" pin="GPIO0" pad="20"/>
<connect gate="G$1" pin="GPIO1" pad="2"/>
<connect gate="G$1" pin="GPIO2" pad="1"/>
<connect gate="G$1" pin="GPIO3" pad="6"/>
<connect gate="G$1" pin="GPIO4" pad="7"/>
<connect gate="G$1" pin="GPIO5" pad="4"/>
<connect gate="G$1" pin="GPIO6" pad="35"/>
<connect gate="G$1" pin="GPIO7" pad="5"/>
<connect gate="G$1" pin="RF_SHDN" pad="21"/>
<connect gate="G$1" pin="RX1" pad="33"/>
<connect gate="G$1" pin="RX2" pad="30"/>
<connect gate="G$1" pin="TX1" pad="32"/>
<connect gate="G$1" pin="TX2" pad="31"/>
<connect gate="G$1" pin="VBAT" pad="23"/>
<connect gate="G$1" pin="VCCIO" pad="28"/>
<connect gate="G$1" pin="VIN_A" pad="8"/>
<connect gate="G$1" pin="VIN_D" pad="26"/>
</connects>
<technologies>
<technology name=""/>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="JACK2.5_SJ-2523" prefix="X">
<description>CUI Inc. SJ-2523-SMT</description>
<gates>
<gate name="G$1" symbol="JACK2.5STEREO"/>
</gates>
<devices>
<device name="" package="JACK2.5_SJ-2523">
<connects>
<connect gate="G$1" pin="MIDDLE" pad="3"/>
<connect gate="G$1" pin="RING" pad="1"/>
<connect gate="G$1" pin="TIP" pad="2"/>
</connects>
<technologies>
<technology name="">
<attribute name="OC_DIGIKEY" value="CP-2523SJCT-ND"/>
</technology>
</technologies>
</device>
<device name="-KLB13" package="LUM_KLB13">
<connects>
<connect gate="G$1" pin="MIDDLE" pad="2"/>
<connect gate="G$1" pin="RING" pad="3"/>
<connect gate="G$1" pin="TIP" pad="1"/>
</connects>
<technologies>
<technology name=""/>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="BA2032" prefix="BAT">
<gates>
<gate name="G$1" symbol="BATTERY2"/>
</gates>
<devices>
<device name="" package="BA2023-ND">
<connects>
<connect gate="G$1" pin="+" pad="P$1 P$2"/>
<connect gate="G$1" pin="-" pad="P$3"/>
</connects>
<technologies>
<technology name="">
<attribute name="OC_DIGIKEY" value="BA2032-ND"/>
</technology>
</technologies>
</device>
<device name="-SM" package="BA2032-SM">
<connects>
<connect gate="G$1" pin="+" pad="+"/>
<connect gate="G$1" pin="-" pad="-"/>
</connects>
<technologies>
<technology name=""/>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="MOLEX_MCX_V">
<description>Molex 73366-0061 / Digi-Key WM5441-ND

MCX straight vertical through-hold 50Ohms</description>
<gates>
<gate name="G$1" symbol="COAX_FGND"/>
<gate name="G$2" symbol="GND"/>
<gate name="G$3" symbol="GND"/>
<gate name="G$4" symbol="GND"/>
</gates>
<devices>
<device name="" package="MOLEX_MCX_V">
<connects>
<connect gate="G$1" pin="1" pad="P$1"/>
<connect gate="G$1" pin="GND" pad="P$2"/>
<connect gate="G$2" pin="GND" pad="P$3"/>
<connect gate="G$3" pin="GND" pad="P$4"/>
<connect gate="G$4" pin="GND" pad="P$5"/>
</connects>
<technologies>
<technology name="">
<attribute name="OC_DIGIKEY" value="WM5441-ND"/>
</technology>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="L-EU0603" uservalue="yes">
<gates>
<gate name="G$1" symbol="L-EU"/>
</gates>
<devices>
<device name="0603" package="0603">
<connects>
<connect gate="G$1" pin="1" pad="1"/>
<connect gate="G$1" pin="2" pad="2"/>
</connects>
<technologies>
<technology name=""/>
</technologies>
</device>
<device name="0402" package="AISC0402">
<connects>
<connect gate="G$1" pin="1" pad="1"/>
<connect gate="G$1" pin="2" pad="2"/>
</connects>
<technologies>
<technology name=""/>
</technologies>
</device>
<device name="1210" package="L1210">
<connects>
<connect gate="G$1" pin="1" pad="1"/>
<connect gate="G$1" pin="2" pad="2"/>
</connects>
<technologies>
<technology name=""/>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="SP3203E">
<description>Exar SP3203E RS232 transceiver with variable CMOS Voltage

Taken from SP3203E_100_120810</description>
<gates>
<gate name="G$1" symbol="SP3203E"/>
</gates>
<devices>
<device name="" package="TSSOP20">
<connects>
<connect gate="G$1" pin="!SHDN" pad="20"/>
<connect gate="G$1" pin="C1+" pad="1"/>
<connect gate="G$1" pin="C1-" pad="3"/>
<connect gate="G$1" pin="C2+" pad="4"/>
<connect gate="G$1" pin="C2-" pad="5"/>
<connect gate="G$1" pin="GND" pad="18"/>
<connect gate="G$1" pin="R1IN" pad="14"/>
<connect gate="G$1" pin="R1OUT" pad="11"/>
<connect gate="G$1" pin="R2IN" pad="13"/>
<connect gate="G$1" pin="R2OUT" pad="10"/>
<connect gate="G$1" pin="T1IN" pad="7"/>
<connect gate="G$1" pin="T1OUT" pad="17"/>
<connect gate="G$1" pin="T2IN" pad="8"/>
<connect gate="G$1" pin="T2OUT" pad="16"/>
<connect gate="G$1" pin="T3IN" pad="9"/>
<connect gate="G$1" pin="T3OUT" pad="15"/>
<connect gate="G$1" pin="V+" pad="2"/>
<connect gate="G$1" pin="V-" pad="6"/>
<connect gate="G$1" pin="VCC" pad="19"/>
<connect gate="G$1" pin="VL" pad="12"/>
</connects>
<technologies>
<technology name="">
<attribute name="OC_DIGIKEY" value="1016-1067-5-ND"/>
</technology>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="74AVC2T45" prefix="IC">
<description>NXP 74AVC2T45 DUAL-BIT, DUAL-SUPPLY VOLTAGE LEVEL TRANSLATOR/TRANSCEIVER; TRI-STATE</description>
<gates>
<gate name="G$1" symbol="74*2T45"/>
</gates>
<devices>
<device name="" package="TSSOP8">
<connects>
<connect gate="G$1" pin="1A" pad="2"/>
<connect gate="G$1" pin="1B" pad="7"/>
<connect gate="G$1" pin="2A" pad="3"/>
<connect gate="G$1" pin="2B" pad="6"/>
<connect gate="G$1" pin="DIR" pad="5"/>
<connect gate="G$1" pin="GND" pad="4"/>
<connect gate="G$1" pin="VCC_A" pad="1"/>
<connect gate="G$1" pin="VCC_B" pad="8"/>
</connects>
<technologies>
<technology name=""/>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="SN74AVC4T245" prefix="IC">
<description>IC @VQFN16: exp pad float or GND</description>
<gates>
<gate name="G$1" symbol="74*4T245"/>
</gates>
<devices>
<device name="" package="TSSOP16">
<connects>
<connect gate="G$1" pin="!1OE" pad="15"/>
<connect gate="G$1" pin="!2OE" pad="14"/>
<connect gate="G$1" pin="1A1" pad="4"/>
<connect gate="G$1" pin="1A2" pad="5"/>
<connect gate="G$1" pin="1B1" pad="13"/>
<connect gate="G$1" pin="1B2" pad="12"/>
<connect gate="G$1" pin="1DIR" pad="2"/>
<connect gate="G$1" pin="2A1" pad="6"/>
<connect gate="G$1" pin="2A2" pad="7"/>
<connect gate="G$1" pin="2B1" pad="11"/>
<connect gate="G$1" pin="2B2" pad="10"/>
<connect gate="G$1" pin="2DIR" pad="3"/>
<connect gate="G$1" pin="GND" pad="9"/>
<connect gate="G$1" pin="GND1" pad="8"/>
<connect gate="G$1" pin="VCC_A" pad="1"/>
<connect gate="G$1" pin="VCC_B" pad="16"/>
</connects>
<technologies>
<technology name="">
<attribute name="OC_DIGIKEY" value="296-18056-1-ND"/>
</technology>
</technologies>
</device>
<device name="-VQFN" package="VQFN-N16">
<connects>
<connect gate="G$1" pin="!1OE" pad="15"/>
<connect gate="G$1" pin="!2OE" pad="14"/>
<connect gate="G$1" pin="1A1" pad="4"/>
<connect gate="G$1" pin="1A2" pad="5"/>
<connect gate="G$1" pin="1B1" pad="13"/>
<connect gate="G$1" pin="1B2" pad="12"/>
<connect gate="G$1" pin="1DIR" pad="2"/>
<connect gate="G$1" pin="2A1" pad="6"/>
<connect gate="G$1" pin="2A2" pad="7"/>
<connect gate="G$1" pin="2B1" pad="11"/>
<connect gate="G$1" pin="2B2" pad="10"/>
<connect gate="G$1" pin="2DIR" pad="3"/>
<connect gate="G$1" pin="GND" pad="9"/>
<connect gate="G$1" pin="GND1" pad="8"/>
<connect gate="G$1" pin="VCC_A" pad="1"/>
<connect gate="G$1" pin="VCC_B" pad="16"/>
</connects>
<technologies>
<technology name=""/>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="SP0503BAHT">
<gates>
<gate name="G$1" symbol="DIODE_ARRAY3"/>
</gates>
<devices>
<device name="" package="SOT143">
<connects>
<connect gate="G$1" pin="A" pad="1"/>
<connect gate="G$1" pin="K" pad="2"/>
<connect gate="G$1" pin="K1" pad="3"/>
<connect gate="G$1" pin="K2" pad="4"/>
</connects>
<technologies>
<technology name="">
<attribute name="OC_DIGIKEY" value="F2715CT-ND"/>
</technology>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="TE_SUBD9M">
<description>TE connectivity 1734351-1</description>
<gates>
<gate name="G$1" symbol="SUBD9M"/>
</gates>
<devices>
<device name="THT" package="DB9_TE">
<connects>
<connect gate="G$1" pin="1" pad="1"/>
<connect gate="G$1" pin="2" pad="2"/>
<connect gate="G$1" pin="3" pad="3"/>
<connect gate="G$1" pin="4" pad="4"/>
<connect gate="G$1" pin="5" pad="5"/>
<connect gate="G$1" pin="6" pad="6"/>
<connect gate="G$1" pin="7" pad="7"/>
<connect gate="G$1" pin="8" pad="8"/>
<connect gate="G$1" pin="9" pad="9"/>
<connect gate="G$1" pin="G1" pad="G1"/>
<connect gate="G$1" pin="G2" pad="G2"/>
</connects>
<technologies>
<technology name=""/>
</technologies>
</device>
<device name="SMD" package="SUBD9M-SMD">
<connects>
<connect gate="G$1" pin="1" pad="1"/>
<connect gate="G$1" pin="2" pad="2"/>
<connect gate="G$1" pin="3" pad="3"/>
<connect gate="G$1" pin="4" pad="4"/>
<connect gate="G$1" pin="5" pad="5"/>
<connect gate="G$1" pin="6" pad="6"/>
<connect gate="G$1" pin="7" pad="7"/>
<connect gate="G$1" pin="8" pad="8"/>
<connect gate="G$1" pin="9" pad="9"/>
<connect gate="G$1" pin="G1" pad="GND1"/>
<connect gate="G$1" pin="G2" pad="GND2"/>
</connects>
<technologies>
<technology name="">
<attribute name="OC_DIGIKEY" value="A35105-ND"/>
</technology>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="SYSMOBTS_PROD">
<description>SysmoBTS Production connector (2x30pin)</description>
<gates>
<gate name="G$1" symbol="SYSMOBTS_PROD_PWR"/>
<gate name="G$2" symbol="SYSMOBTS_PROD_SPI"/>
<gate name="G$3" symbol="SYSMOBTS_PROD_FPGA_JTAG"/>
<gate name="G$4" symbol="SYSMOBTS_PROD_DSP_JTAG"/>
<gate name="G$5" symbol="SYSMOBTS_CPLD_JTAG"/>
</gates>
<devices>
<device name="" package="HSEC8-130-01-X-DV-A">
<connects>
<connect gate="G$1" pin="1V2CORE_1" pad="B13"/>
<connect gate="G$1" pin="1V2CORE_2" pad="B14"/>
<connect gate="G$1" pin="1V2DC_1" pad="B10"/>
<connect gate="G$1" pin="1V2DC_2" pad="B11"/>
<connect gate="G$1" pin="1V8DC_1" pad="B7"/>
<connect gate="G$1" pin="1V8DC_2" pad="B8"/>
<connect gate="G$1" pin="3V3DC_1" pad="B4"/>
<connect gate="G$1" pin="3V3DC_2" pad="B5"/>
<connect gate="G$1" pin="5VDC_1" pad="B1"/>
<connect gate="G$1" pin="5VDC_2" pad="B2"/>
<connect gate="G$1" pin="GND1" pad="B16"/>
<connect gate="G$1" pin="GND2" pad="B17"/>
<connect gate="G$1" pin="GND3" pad="B18"/>
<connect gate="G$1" pin="GND4" pad="B19"/>
<connect gate="G$1" pin="GND5" pad="B20"/>
<connect gate="G$2" pin="DSP_BTSEL0" pad="A2"/>
<connect gate="G$2" pin="DSP_BTSEL1" pad="A1"/>
<connect gate="G$2" pin="GND1" pad="A3"/>
<connect gate="G$2" pin="GND2" pad="A6"/>
<connect gate="G$2" pin="I2C_SCL" pad="A7"/>
<connect gate="G$2" pin="I2C_SDA" pad="A8"/>
<connect gate="G$2" pin="SPICLK" pad="B25"/>
<connect gate="G$2" pin="SPIDI" pad="B28"/>
<connect gate="G$2" pin="SPIDO" pad="B29"/>
<connect gate="G$2" pin="SPIEN0" pad="B27"/>
<connect gate="G$2" pin="SPIEN1" pad="B26"/>
<connect gate="G$2" pin="UART_RX0" pad="A5"/>
<connect gate="G$2" pin="UART_TX0" pad="A4"/>
<connect gate="G$3" pin="FPGA_GND" pad="A14"/>
<connect gate="G$3" pin="FPGA_TCK" pad="A12"/>
<connect gate="G$3" pin="FPGA_TDI" pad="A10"/>
<connect gate="G$3" pin="FPGA_TDO" pad="A11"/>
<connect gate="G$3" pin="FPGA_TMS" pad="A13"/>
<connect gate="G$4" pin="DSP_EMU0" pad="A21"/>
<connect gate="G$4" pin="DSP_EMU1" pad="A22"/>
<connect gate="G$4" pin="DSP_GND" pad="A23"/>
<connect gate="G$4" pin="DSP_RTCK" pad="A19"/>
<connect gate="G$4" pin="DSP_TCK" pad="A20"/>
<connect gate="G$4" pin="DSP_TDI" pad="A17"/>
<connect gate="G$4" pin="DSP_TDO" pad="A18"/>
<connect gate="G$4" pin="DSP_TMS" pad="A15"/>
<connect gate="G$4" pin="DSP_TRST" pad="A16"/>
<connect gate="G$5" pin="CPLD_GND" pad="A28"/>
<connect gate="G$5" pin="CPLD_TCK" pad="A24"/>
<connect gate="G$5" pin="CPLD_TDI" pad="A25"/>
<connect gate="G$5" pin="CPLD_TDO" pad="A26"/>
<connect gate="G$5" pin="CPLD_TMS" pad="A27"/>
</connects>
<technologies>
<technology name=""/>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="IDT_ICS501">
<gates>
<gate name="G$1" symbol="IDT_ICS501"/>
</gates>
<devices>
<device name="" package="SOIC08">
<connects>
<connect gate="G$1" pin="CLK" pad="5"/>
<connect gate="G$1" pin="GND" pad="3"/>
<connect gate="G$1" pin="OE" pad="7"/>
<connect gate="G$1" pin="S0" pad="6"/>
<connect gate="G$1" pin="S1" pad="4"/>
<connect gate="G$1" pin="VCC" pad="2"/>
<connect gate="G$1" pin="X1_ICLK" pad="1"/>
<connect gate="G$1" pin="X2" pad="8"/>
</connects>
<technologies>
<technology name="">
<attribute name="OC_DIGIKEY" value="800-1036-1-ND"/>
</technology>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="PINHD-1X6" prefix="JP" uservalue="yes">
<description>&lt;b&gt;PIN HEADER&lt;/b&gt;</description>
<gates>
<gate name="A" symbol="REBELFPC_CON"/>
</gates>
<devices>
<device name="" package="1X06">
<connects>
<connect gate="A" pin="!RST" pad="2"/>
<connect gate="A" pin="CLK" pad="3"/>
<connect gate="A" pin="GND" pad="6"/>
<connect gate="A" pin="I/O" pad="4"/>
<connect gate="A" pin="VCC" pad="1"/>
<connect gate="A" pin="VPP" pad="5"/>
</connects>
<technologies>
<technology name=""/>
</technologies>
</device>
<device name="/90" package="1X06/90">
<connects>
<connect gate="A" pin="!RST" pad="2"/>
<connect gate="A" pin="CLK" pad="3"/>
<connect gate="A" pin="GND" pad="6"/>
<connect gate="A" pin="I/O" pad="4"/>
<connect gate="A" pin="VCC" pad="1"/>
<connect gate="A" pin="VPP" pad="5"/>
</connects>
<technologies>
<technology name=""/>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="FCI_FPC_REBEL_SFW6R-1">
<gates>
<gate name="G$1" symbol="REBELFPC_CON"/>
</gates>
<devices>
<device name="" package="FPC_REBEL_SFW6R-1ST">
<connects>
<connect gate="G$1" pin="!RST" pad="2"/>
<connect gate="G$1" pin="CLK" pad="3"/>
<connect gate="G$1" pin="GND" pad="6"/>
<connect gate="G$1" pin="I/O" pad="4"/>
<connect gate="G$1" pin="VCC" pad="1"/>
<connect gate="G$1" pin="VPP" pad="5"/>
</connects>
<technologies>
<technology name="">
<attribute name="OC_DIGIKEY" value="609-1889-1-ND"/>
</technology>
</technologies>
</device>
<device name="SOLDER" package="FPC_SODLER_6">
<connects>
<connect gate="G$1" pin="!RST" pad="1"/>
<connect gate="G$1" pin="CLK" pad="2"/>
<connect gate="G$1" pin="GND" pad="3"/>
<connect gate="G$1" pin="I/O" pad="4"/>
<connect gate="G$1" pin="VCC" pad="5"/>
<connect gate="G$1" pin="VPP" pad="6"/>
</connects>
<technologies>
<technology name=""/>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="PINHD-1X2" prefix="JP" uservalue="yes">
<description>&lt;b&gt;PIN HEADER&lt;/b&gt;</description>
<gates>
<gate name="G$1" symbol="PINHD2"/>
</gates>
<devices>
<device name="" package="1X02">
<connects>
<connect gate="G$1" pin="1" pad="1"/>
<connect gate="G$1" pin="2" pad="2"/>
</connects>
<technologies>
<technology name=""/>
</technologies>
</device>
<device name="/90" package="1X02/90">
<connects>
<connect gate="G$1" pin="1" pad="1"/>
<connect gate="G$1" pin="2" pad="2"/>
</connects>
<technologies>
<technology name=""/>
</technologies>
</device>
<device name="SMD" package="1X02_SMD">
<connects>
<connect gate="G$1" pin="1" pad="1"/>
<connect gate="G$1" pin="2" pad="2"/>
</connects>
<technologies>
<technology name=""/>
</technologies>
</device>
<device name="SMD90" package="1X2_SMD_90">
<connects>
<connect gate="G$1" pin="1" pad="P$1"/>
<connect gate="G$1" pin="2" pad="P$2"/>
</connects>
<technologies>
<technology name=""/>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="PINHD-2X10" prefix="JP" uservalue="yes">
<description>&lt;b&gt;PIN HEADER&lt;/b&gt;</description>
<gates>
<gate name="A" symbol="PINH2X10"/>
</gates>
<devices>
<device name="" package="2X10">
<connects>
<connect gate="A" pin="1" pad="1"/>
<connect gate="A" pin="10" pad="10"/>
<connect gate="A" pin="11" pad="11"/>
<connect gate="A" pin="12" pad="12"/>
<connect gate="A" pin="13" pad="13"/>
<connect gate="A" pin="14" pad="14"/>
<connect gate="A" pin="15" pad="15"/>
<connect gate="A" pin="16" pad="16"/>
<connect gate="A" pin="17" pad="17"/>
<connect gate="A" pin="18" pad="18"/>
<connect gate="A" pin="19" pad="19"/>
<connect gate="A" pin="2" pad="2"/>
<connect gate="A" pin="20" pad="20"/>
<connect gate="A" pin="3" pad="3"/>
<connect gate="A" pin="4" pad="4"/>
<connect gate="A" pin="5" pad="5"/>
<connect gate="A" pin="6" pad="6"/>
<connect gate="A" pin="7" pad="7"/>
<connect gate="A" pin="8" pad="8"/>
<connect gate="A" pin="9" pad="9"/>
</connects>
<technologies>
<technology name=""/>
</technologies>
</device>
<device name="/90" package="2X10/90">
<connects>
<connect gate="A" pin="1" pad="1"/>
<connect gate="A" pin="10" pad="10"/>
<connect gate="A" pin="11" pad="11"/>
<connect gate="A" pin="12" pad="12"/>
<connect gate="A" pin="13" pad="13"/>
<connect gate="A" pin="14" pad="14"/>
<connect gate="A" pin="15" pad="15"/>
<connect gate="A" pin="16" pad="16"/>
<connect gate="A" pin="17" pad="17"/>
<connect gate="A" pin="18" pad="18"/>
<connect gate="A" pin="19" pad="19"/>
<connect gate="A" pin="2" pad="2"/>
<connect gate="A" pin="20" pad="20"/>
<connect gate="A" pin="3" pad="3"/>
<connect gate="A" pin="4" pad="4"/>
<connect gate="A" pin="5" pad="5"/>
<connect gate="A" pin="6" pad="6"/>
<connect gate="A" pin="7" pad="7"/>
<connect gate="A" pin="8" pad="8"/>
<connect gate="A" pin="9" pad="9"/>
</connects>
<technologies>
<technology name=""/>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="PINHD-2X20" prefix="JP" uservalue="yes">
<description>&lt;b&gt;PIN HEADER&lt;/b&gt;</description>
<gates>
<gate name="A" symbol="PINH2X20"/>
</gates>
<devices>
<device name="" package="2X20">
<connects>
<connect gate="A" pin="1" pad="1"/>
<connect gate="A" pin="10" pad="10"/>
<connect gate="A" pin="11" pad="11"/>
<connect gate="A" pin="12" pad="12"/>
<connect gate="A" pin="13" pad="13"/>
<connect gate="A" pin="14" pad="14"/>
<connect gate="A" pin="15" pad="15"/>
<connect gate="A" pin="16" pad="16"/>
<connect gate="A" pin="17" pad="17"/>
<connect gate="A" pin="18" pad="18"/>
<connect gate="A" pin="19" pad="19"/>
<connect gate="A" pin="2" pad="2"/>
<connect gate="A" pin="20" pad="20"/>
<connect gate="A" pin="21" pad="21"/>
<connect gate="A" pin="22" pad="22"/>
<connect gate="A" pin="23" pad="23"/>
<connect gate="A" pin="24" pad="24"/>
<connect gate="A" pin="25" pad="25"/>
<connect gate="A" pin="26" pad="26"/>
<connect gate="A" pin="27" pad="27"/>
<connect gate="A" pin="28" pad="28"/>
<connect gate="A" pin="29" pad="29"/>
<connect gate="A" pin="3" pad="3"/>
<connect gate="A" pin="30" pad="30"/>
<connect gate="A" pin="31" pad="31"/>
<connect gate="A" pin="32" pad="32"/>
<connect gate="A" pin="33" pad="33"/>
<connect gate="A" pin="34" pad="34"/>
<connect gate="A" pin="35" pad="35"/>
<connect gate="A" pin="36" pad="36"/>
<connect gate="A" pin="37" pad="37"/>
<connect gate="A" pin="38" pad="38"/>
<connect gate="A" pin="39" pad="39"/>
<connect gate="A" pin="4" pad="4"/>
<connect gate="A" pin="40" pad="40"/>
<connect gate="A" pin="5" pad="5"/>
<connect gate="A" pin="6" pad="6"/>
<connect gate="A" pin="7" pad="7"/>
<connect gate="A" pin="8" pad="8"/>
<connect gate="A" pin="9" pad="9"/>
</connects>
<technologies>
<technology name=""/>
</technologies>
</device>
<device name="/90" package="2X20/90">
<connects>
<connect gate="A" pin="1" pad="1"/>
<connect gate="A" pin="10" pad="10"/>
<connect gate="A" pin="11" pad="11"/>
<connect gate="A" pin="12" pad="12"/>
<connect gate="A" pin="13" pad="13"/>
<connect gate="A" pin="14" pad="14"/>
<connect gate="A" pin="15" pad="15"/>
<connect gate="A" pin="16" pad="16"/>
<connect gate="A" pin="17" pad="17"/>
<connect gate="A" pin="18" pad="18"/>
<connect gate="A" pin="19" pad="19"/>
<connect gate="A" pin="2" pad="2"/>
<connect gate="A" pin="20" pad="20"/>
<connect gate="A" pin="21" pad="21"/>
<connect gate="A" pin="22" pad="22"/>
<connect gate="A" pin="23" pad="23"/>
<connect gate="A" pin="24" pad="24"/>
<connect gate="A" pin="25" pad="25"/>
<connect gate="A" pin="26" pad="26"/>
<connect gate="A" pin="27" pad="27"/>
<connect gate="A" pin="28" pad="28"/>
<connect gate="A" pin="29" pad="29"/>
<connect gate="A" pin="3" pad="3"/>
<connect gate="A" pin="30" pad="30"/>
<connect gate="A" pin="31" pad="31"/>
<connect gate="A" pin="32" pad="32"/>
<connect gate="A" pin="33" pad="33"/>
<connect gate="A" pin="34" pad="34"/>
<connect gate="A" pin="35" pad="35"/>
<connect gate="A" pin="36" pad="36"/>
<connect gate="A" pin="37" pad="37"/>
<connect gate="A" pin="38" pad="38"/>
<connect gate="A" pin="39" pad="39"/>
<connect gate="A" pin="4" pad="4"/>
<connect gate="A" pin="40" pad="40"/>
<connect gate="A" pin="5" pad="5"/>
<connect gate="A" pin="6" pad="6"/>
<connect gate="A" pin="7" pad="7"/>
<connect gate="A" pin="8" pad="8"/>
<connect gate="A" pin="9" pad="9"/>
</connects>
<technologies>
<technology name=""/>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="PINHD-2X5" prefix="X" uservalue="yes">
<description>&lt;b&gt;PIN HEADER&lt;/b&gt;</description>
<gates>
<gate name="A" symbol="PINH2X5"/>
</gates>
<devices>
<device name="" package="2X05">
<connects>
<connect gate="A" pin="1" pad="1"/>
<connect gate="A" pin="10" pad="10"/>
<connect gate="A" pin="2" pad="2"/>
<connect gate="A" pin="3" pad="3"/>
<connect gate="A" pin="4" pad="4"/>
<connect gate="A" pin="5" pad="5"/>
<connect gate="A" pin="6" pad="6"/>
<connect gate="A" pin="7" pad="7"/>
<connect gate="A" pin="8" pad="8"/>
<connect gate="A" pin="9" pad="9"/>
</connects>
<technologies>
<technology name=""/>
</technologies>
</device>
<device name="/90" package="2X05/90">
<connects>
<connect gate="A" pin="1" pad="1"/>
<connect gate="A" pin="10" pad="10"/>
<connect gate="A" pin="2" pad="2"/>
<connect gate="A" pin="3" pad="3"/>
<connect gate="A" pin="4" pad="4"/>
<connect gate="A" pin="5" pad="5"/>
<connect gate="A" pin="6" pad="6"/>
<connect gate="A" pin="7" pad="7"/>
<connect gate="A" pin="8" pad="8"/>
<connect gate="A" pin="9" pad="9"/>
</connects>
<technologies>
<technology name=""/>
</technologies>
</device>
<device name="-SMD90" package="2X05_SMD_90">
<connects>
<connect gate="A" pin="1" pad="1"/>
<connect gate="A" pin="10" pad="10"/>
<connect gate="A" pin="2" pad="2"/>
<connect gate="A" pin="3" pad="3"/>
<connect gate="A" pin="4" pad="4"/>
<connect gate="A" pin="5" pad="5"/>
<connect gate="A" pin="6" pad="6"/>
<connect gate="A" pin="7" pad="7"/>
<connect gate="A" pin="8" pad="8"/>
<connect gate="A" pin="9" pad="9"/>
</connects>
<technologies>
<technology name=""/>
</technologies>
</device>
<device name="-SMD180" package="2X05_SMD_180">
<connects>
<connect gate="A" pin="1" pad="1"/>
<connect gate="A" pin="10" pad="10"/>
<connect gate="A" pin="2" pad="2"/>
<connect gate="A" pin="3" pad="3"/>
<connect gate="A" pin="4" pad="4"/>
<connect gate="A" pin="5" pad="5"/>
<connect gate="A" pin="6" pad="6"/>
<connect gate="A" pin="7" pad="7"/>
<connect gate="A" pin="8" pad="8"/>
<connect gate="A" pin="9" pad="9"/>
</connects>
<technologies>
<technology name=""/>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="SC16IS740">
<description>NXP SC16IS740 SPI/I2C UART</description>
<gates>
<gate name="G$1" symbol="SC16IS740"/>
</gates>
<devices>
<device name="" package="TSSOP16L">
<connects>
<connect gate="G$1" pin="!CS" pad="2"/>
<connect gate="G$1" pin="!CTS" pad="11"/>
<connect gate="G$1" pin="!IRQ" pad="7"/>
<connect gate="G$1" pin="!RESET" pad="14"/>
<connect gate="G$1" pin="!RTS" pad="10"/>
<connect gate="G$1" pin="!SPI" pad="8"/>
<connect gate="G$1" pin="RX" pad="13"/>
<connect gate="G$1" pin="SCLK" pad="5"/>
<connect gate="G$1" pin="SI" pad="3"/>
<connect gate="G$1" pin="SO" pad="4"/>
<connect gate="G$1" pin="TX" pad="12"/>
<connect gate="G$1" pin="VDD" pad="1"/>
<connect gate="G$1" pin="VSS" pad="6"/>
<connect gate="G$1" pin="VSS2" pad="9"/>
<connect gate="G$1" pin="XTAL1" pad="15"/>
<connect gate="G$1" pin="XTAL2" pad="16"/>
</connects>
<technologies>
<technology name="">
<attribute name="OC_DIGIKEY" value="568-6674-1-ND"/>
</technology>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="PINHD-1X8" prefix="JP" uservalue="yes">
<description>&lt;b&gt;PIN HEADER&lt;/b&gt;</description>
<gates>
<gate name="A" symbol="PINHD8"/>
</gates>
<devices>
<device name="" package="1X08">
<connects>
<connect gate="A" pin="1" pad="1"/>
<connect gate="A" pin="2" pad="2"/>
<connect gate="A" pin="3" pad="3"/>
<connect gate="A" pin="4" pad="4"/>
<connect gate="A" pin="5" pad="5"/>
<connect gate="A" pin="6" pad="6"/>
<connect gate="A" pin="7" pad="7"/>
<connect gate="A" pin="8" pad="8"/>
</connects>
<technologies>
<technology name=""/>
</technologies>
</device>
<device name="/90" package="1X08/90">
<connects>
<connect gate="A" pin="1" pad="1"/>
<connect gate="A" pin="2" pad="2"/>
<connect gate="A" pin="3" pad="3"/>
<connect gate="A" pin="4" pad="4"/>
<connect gate="A" pin="5" pad="5"/>
<connect gate="A" pin="6" pad="6"/>
<connect gate="A" pin="7" pad="7"/>
<connect gate="A" pin="8" pad="8"/>
</connects>
<technologies>
<technology name=""/>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="SW_DIP_SMD-02">
<gates>
<gate name="SW$1" symbol="SW_DIP-02"/>
</gates>
<devices>
<device name="" package="DIP_SW_SMD-02">
<connects>
<connect gate="SW$1" pin="1" pad="P$1"/>
<connect gate="SW$1" pin="2" pad="P$2"/>
<connect gate="SW$1" pin="3" pad="P$3"/>
<connect gate="SW$1" pin="4" pad="P$4"/>
</connects>
<technologies>
<technology name="">
<attribute name="OC_DIGIKEY" value="CT2192MST-ND"/>
</technology>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="WAVECOM_Q268X">
<description>Wavecom Q2686/Q2687 GSM/GPRS Modem</description>
<gates>
<gate name="G$1" symbol="WAVECOM_Q268X_PS"/>
<gate name="G$2" symbol="WAVECOM_Q268X_SIM"/>
<gate name="G$3" symbol="WAVECOM_Q268X_AUDIO"/>
<gate name="G$4" symbol="WAVECOM_Q268X_RS232"/>
<gate name="G$5" symbol="WAVECOM_Q268X_PCM"/>
<gate name="G$6" symbol="WAVECOM_Q268X_USB"/>
<gate name="G$7" symbol="WAVECOM_Q268X_MISC"/>
<gate name="G$8" symbol="WAVECOM_Q268X_SPI"/>
</gates>
<devices>
<device name="" package="WAVECOM_Q26">
<connects>
<connect gate="G$1" pin="BAT_RTC" pad="7"/>
<connect gate="G$1" pin="CHG_IN1" pad="6"/>
<connect gate="G$1" pin="CHG_IN2" pad="8"/>
<connect gate="G$1" pin="GND1" pad="G1"/>
<connect gate="G$1" pin="GND2" pad="G2"/>
<connect gate="G$1" pin="GND3" pad="G3"/>
<connect gate="G$1" pin="GND4" pad="G4"/>
<connect gate="G$1" pin="VBATT1" pad="1"/>
<connect gate="G$1" pin="VBATT2" pad="2"/>
<connect gate="G$1" pin="VBATT3" pad="3"/>
<connect gate="G$1" pin="VBATT4" pad="4"/>
<connect gate="G$2" pin="!SIM_RST" pad="13"/>
<connect gate="G$2" pin="SIMPRES" pad="12"/>
<connect gate="G$2" pin="SIM_CLK" pad="14"/>
<connect gate="G$2" pin="SIM_IO" pad="11"/>
<connect gate="G$2" pin="SIM_VCC" pad="9"/>
<connect gate="G$3" pin="MIC1N" pad="38"/>
<connect gate="G$3" pin="MIC1P" pad="40"/>
<connect gate="G$3" pin="MIC2N" pad="34"/>
<connect gate="G$3" pin="MIC2P" pad="36"/>
<connect gate="G$3" pin="SPK1N" pad="37"/>
<connect gate="G$3" pin="SPK1P" pad="35"/>
<connect gate="G$3" pin="SPK2N" pad="41"/>
<connect gate="G$3" pin="SPK2P" pad="39"/>
<connect gate="G$4" pin="!CTS" pad="75"/>
<connect gate="G$4" pin="!CTS2" pad="32"/>
<connect gate="G$4" pin="!DCD" pad="70"/>
<connect gate="G$4" pin="!DSR" pad="74"/>
<connect gate="G$4" pin="!DTR" pad="76"/>
<connect gate="G$4" pin="!RI" pad="69"/>
<connect gate="G$4" pin="!RTS" pad="72"/>
<connect gate="G$4" pin="!RTS2" pad="33"/>
<connect gate="G$4" pin="RXD" pad="73"/>
<connect gate="G$4" pin="RXD2" pad="30"/>
<connect gate="G$4" pin="TXD" pad="71"/>
<connect gate="G$4" pin="TXD2" pad="31"/>
<connect gate="G$5" pin="PCM_CLK" pad="79"/>
<connect gate="G$5" pin="PCM_IN" pad="78"/>
<connect gate="G$5" pin="PCM_OUT" pad="80"/>
<connect gate="G$5" pin="PCM_SYNC" pad="77"/>
<connect gate="G$6" pin="USB_DN" pad="56"/>
<connect gate="G$6" pin="USB_DP" pad="54"/>
<connect gate="G$6" pin="VPAD_USB" pad="52"/>
<connect gate="G$7" pin="!RESET" pad="18"/>
<connect gate="G$7" pin="ADC2" pad="21"/>
<connect gate="G$7" pin="BAT_TEMP" pad="20"/>
<connect gate="G$7" pin="BOOT" pad="16"/>
<connect gate="G$7" pin="BUZZER" pad="15"/>
<connect gate="G$7" pin="LED0" pad="17"/>
<connect gate="G$7" pin="ON_!OFF" pad="19"/>
<connect gate="G$7" pin="VCC_1V8" pad="5"/>
<connect gate="G$7" pin="VCC_2V8" pad="10"/>
<connect gate="G$8" pin="GPIO0" pad="43"/>
<connect gate="G$8" pin="GPIO1" pad="51"/>
<connect gate="G$8" pin="GPIO19" pad="45"/>
<connect gate="G$8" pin="GPIO2" pad="53"/>
<connect gate="G$8" pin="GPIO20" pad="48"/>
<connect gate="G$8" pin="GPIO21" pad="47"/>
<connect gate="G$8" pin="GPIO22" pad="57"/>
<connect gate="G$8" pin="GPIO23" pad="55"/>
<connect gate="G$8" pin="GPIO24" pad="58"/>
<connect gate="G$8" pin="GPIO25/INT1" pad="49"/>
<connect gate="G$8" pin="GPIO3/INT0" pad="50"/>
<connect gate="G$8" pin="GPIO31" pad="22"/>
<connect gate="G$8" pin="GPIO35" pad="28"/>
<connect gate="G$8" pin="I2C_SCL" pad="44"/>
<connect gate="G$8" pin="I2C_SDA" pad="46"/>
<connect gate="G$8" pin="SPI1_CLK" pad="23"/>
<connect gate="G$8" pin="SPI1_I" pad="24"/>
<connect gate="G$8" pin="SPI1_IO" pad="25"/>
<connect gate="G$8" pin="SPI2_CLK" pad="26"/>
<connect gate="G$8" pin="SPI2_I" pad="29"/>
<connect gate="G$8" pin="SPI2_IO" pad="27"/>
</connects>
<technologies>
<technology name=""/>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="MAX3218">
<gates>
<gate name="G$1" symbol="MAX3218"/>
</gates>
<devices>
<device name="" package="SSOP20">
<connects>
<connect gate="G$1" pin="!FORCEOFF" pad="4"/>
<connect gate="G$1" pin="!INVALID" pad="2"/>
<connect gate="G$1" pin="C1N" pad="16"/>
<connect gate="G$1" pin="C1P" pad="18"/>
<connect gate="G$1" pin="FORCEON" pad="3"/>
<connect gate="G$1" pin="GND" pad="5"/>
<connect gate="G$1" pin="GND2" pad="17"/>
<connect gate="G$1" pin="GND3" pad="20"/>
<connect gate="G$1" pin="LX" pad="1"/>
<connect gate="G$1" pin="R1IN" pad="12"/>
<connect gate="G$1" pin="R1OUT" pad="9"/>
<connect gate="G$1" pin="R2IN" pad="11"/>
<connect gate="G$1" pin="R2OUT" pad="10"/>
<connect gate="G$1" pin="T1IN" pad="7"/>
<connect gate="G$1" pin="T1OUT" pad="14"/>
<connect gate="G$1" pin="T2IN" pad="8"/>
<connect gate="G$1" pin="T2OUT" pad="13"/>
<connect gate="G$1" pin="VCC" pad="6"/>
<connect gate="G$1" pin="VN" pad="15"/>
<connect gate="G$1" pin="VP" pad="19"/>
</connects>
<technologies>
<technology name="">
<attribute name="OC_DIGIKEY" value="MAX3218CAP+-ND"/>
</technology>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="L-EU1210" uservalue="yes">
<gates>
<gate name="L$1" symbol="L-EU"/>
</gates>
<devices>
<device name="" package="L1210">
<connects>
<connect gate="L$1" pin="1" pad="2"/>
<connect gate="L$1" pin="2" pad="1"/>
</connects>
<technologies>
<technology name=""/>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="0603ESDA-TR" prefix="D">
<description>Bussmann 0603ESDA-TR ESD Suppressor</description>
<gates>
<gate name="G$1" symbol="ESD_TVS_DIODE"/>
</gates>
<devices>
<device name="" package="0603">
<connects>
<connect gate="G$1" pin="A" pad="1"/>
<connect gate="G$1" pin="K" pad="2"/>
</connects>
<technologies>
<technology name=""/>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="PINHD_1X3" prefix="X">
<gates>
<gate name="G$1" symbol="PINHD3"/>
</gates>
<devices>
<device name="" package="1X3_SMD_90">
<connects>
<connect gate="G$1" pin="1" pad="P$1"/>
<connect gate="G$1" pin="2" pad="P$2"/>
<connect gate="G$1" pin="3" pad="P$3"/>
</connects>
<technologies>
<technology name=""/>
</technologies>
</device>
<device name="SMD" package="1X03_SMD">
<connects>
<connect gate="G$1" pin="1" pad="1"/>
<connect gate="G$1" pin="2" pad="2"/>
<connect gate="G$1" pin="3" pad="3"/>
</connects>
<technologies>
<technology name=""/>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="MAX3322E">
<description>Maxim MAX3322E - 15kV ESD-Protected, RS232 Transceiver for multidrop</description>
<gates>
<gate name="G$1" symbol="MAX3322E"/>
</gates>
<devices>
<device name="" package="TSSOP20">
<connects>
<connect gate="G$1" pin="!SHDN" pad="18"/>
<connect gate="G$1" pin="C1N" pad="3"/>
<connect gate="G$1" pin="C1P" pad="1"/>
<connect gate="G$1" pin="C2N" pad="5"/>
<connect gate="G$1" pin="C2P" pad="4"/>
<connect gate="G$1" pin="GND" pad="19"/>
<connect gate="G$1" pin="R1IN" pad="10"/>
<connect gate="G$1" pin="R1OUT" pad="11"/>
<connect gate="G$1" pin="R2IN" pad="8"/>
<connect gate="G$1" pin="R2OUT" pad="13"/>
<connect gate="G$1" pin="RENABLE" pad="16"/>
<connect gate="G$1" pin="T1IN" pad="12"/>
<connect gate="G$1" pin="T1OUT" pad="9"/>
<connect gate="G$1" pin="T2IN" pad="14"/>
<connect gate="G$1" pin="T2OUT" pad="7"/>
<connect gate="G$1" pin="TXENABLE" pad="15"/>
<connect gate="G$1" pin="VCC" pad="20"/>
<connect gate="G$1" pin="VL" pad="17"/>
<connect gate="G$1" pin="VN" pad="6"/>
<connect gate="G$1" pin="VP" pad="2"/>
</connects>
<technologies>
<technology name="">
<attribute name="OC_DIGIKEY" value="MAX3322EEUP+-ND"/>
</technology>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="CTS_OSC_4PAD">
<description>CTS Model 636 ceramic packaged clock oscillator

CTS Electronic Components, Inc</description>
<gates>
<gate name="G$1" symbol="QG1"/>
</gates>
<devices>
<device name="" package="CTS_4SMD">
<connects>
<connect gate="G$1" pin="FO" pad="3"/>
<connect gate="G$1" pin="GND" pad="2"/>
<connect gate="G$1" pin="OE" pad="1"/>
<connect gate="G$1" pin="VCC" pad="4"/>
</connects>
<technologies>
<technology name=""/>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="NHD-C0216CIZ">
<description>NHD-C0216CiZ-FSW-FBW-3V3</description>
<gates>
<gate name="G$1" symbol="LCD"/>
</gates>
<devices>
<device name="" package="NHD-C0216CIZ-FSW-FBW-3V3">
<connects>
<connect gate="G$1" pin="!RST" pad="1"/>
<connect gate="G$1" pin="C+" pad="7"/>
<connect gate="G$1" pin="C-" pad="8"/>
<connect gate="G$1" pin="GND" pad="4"/>
<connect gate="G$1" pin="LED+" pad="A"/>
<connect gate="G$1" pin="LED-" pad="K"/>
<connect gate="G$1" pin="SCL" pad="2"/>
<connect gate="G$1" pin="SDA" pad="3"/>
<connect gate="G$1" pin="VDD" pad="5"/>
<connect gate="G$1" pin="VOUT" pad="6"/>
</connects>
<technologies>
<technology name="">
<attribute name="OC_DIGIKEY" value="NHD-C0216CZ-FSW-FBW-3V3-ND"/>
</technology>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="DIP_SP6T">
<description>DIP SP6T switch COPAL SS-10-16</description>
<gates>
<gate name="G$1" symbol="SP6T"/>
</gates>
<devices>
<device name="" package="DIP_SP6T">
<connects>
<connect gate="G$1" pin="1" pad="1"/>
<connect gate="G$1" pin="2" pad="2"/>
<connect gate="G$1" pin="3" pad="3"/>
<connect gate="G$1" pin="4" pad="4"/>
<connect gate="G$1" pin="5" pad="5"/>
<connect gate="G$1" pin="6" pad="6"/>
<connect gate="G$1" pin="C" pad="C"/>
</connects>
<technologies>
<technology name=""/>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="SWITCH_4PDT">
<gates>
<gate name="G$1" symbol="SW_4PDT"/>
</gates>
<devices>
<device name="" package="4PDT_DIL12">
<connects>
<connect gate="G$1" pin="A" pad="A"/>
<connect gate="G$1" pin="A1" pad="A1"/>
<connect gate="G$1" pin="A2" pad="A2"/>
<connect gate="G$1" pin="B" pad="B"/>
<connect gate="G$1" pin="B1" pad="B1"/>
<connect gate="G$1" pin="B2" pad="B2"/>
<connect gate="G$1" pin="C" pad="C"/>
<connect gate="G$1" pin="C1" pad="C1"/>
<connect gate="G$1" pin="C2" pad="C2"/>
<connect gate="G$1" pin="D" pad="D"/>
<connect gate="G$1" pin="D1" pad="D1"/>
<connect gate="G$1" pin="D2" pad="D2"/>
</connects>
<technologies>
<technology name="">
<attribute name="OC_DIGIKEY" value="450-1633-ND"/>
</technology>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="MICROSTACK_12">
<gates>
<gate name="G$1" symbol="PINH2X6"/>
</gates>
<devices>
<device name="" package="MOLEX_MICROSTACK_12PIN">
<connects>
<connect gate="G$1" pin="1" pad="1"/>
<connect gate="G$1" pin="10" pad="10"/>
<connect gate="G$1" pin="11" pad="11"/>
<connect gate="G$1" pin="12" pad="12"/>
<connect gate="G$1" pin="2" pad="2"/>
<connect gate="G$1" pin="3" pad="3"/>
<connect gate="G$1" pin="4" pad="4"/>
<connect gate="G$1" pin="5" pad="5"/>
<connect gate="G$1" pin="6" pad="6"/>
<connect gate="G$1" pin="7" pad="7"/>
<connect gate="G$1" pin="8" pad="8"/>
<connect gate="G$1" pin="9" pad="9"/>
</connects>
<technologies>
<technology name=""/>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="FPC6">
<gates>
<gate name="G$1" symbol="PINHD6"/>
</gates>
<devices>
<device name="" package="FPC_SODLER_6">
<connects>
<connect gate="G$1" pin="1" pad="1"/>
<connect gate="G$1" pin="2" pad="2"/>
<connect gate="G$1" pin="3" pad="3"/>
<connect gate="G$1" pin="4" pad="4"/>
<connect gate="G$1" pin="5" pad="5"/>
<connect gate="G$1" pin="6" pad="6"/>
</connects>
<technologies>
<technology name=""/>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="I4S_DEBUG">
<description>iPhone 4S Debug Connector (adapter side, not phone side)</description>
<gates>
<gate name="G$1" symbol="I4S_DEBUG"/>
</gates>
<devices>
<device name="" package="AXE580124">
<connects>
<connect gate="G$1" pin="!BB_JTAG_TRST_N" pad="34"/>
<connect gate="G$1" pin="!BB_UART_CTS_N" pad="70"/>
<connect gate="G$1" pin="!BB_UART_RTS_N" pad="68"/>
<connect gate="G$1" pin="!BT_RESET_N" pad="15"/>
<connect gate="G$1" pin="!BT_UART_CTS_N" pad="25"/>
<connect gate="G$1" pin="!BT_UART_RTS_N" pad="23"/>
<connect gate="G$1" pin="!DEBUG_RST_N" pad="10"/>
<connect gate="G$1" pin="!RADIO_ON_N" pad="14"/>
<connect gate="G$1" pin="!RESET_PMU_N" pad="12"/>
<connect gate="G$1" pin="!RF_RESET_N" pad="11"/>
<connect gate="G$1" pin="BATT_VCC1" pad="1"/>
<connect gate="G$1" pin="BATT_VCC2" pad="2"/>
<connect gate="G$1" pin="BATT_VCC3" pad="3"/>
<connect gate="G$1" pin="BATT_VCC4" pad="4"/>
<connect gate="G$1" pin="BATT_VCC5" pad="5"/>
<connect gate="G$1" pin="BATT_VCC6" pad="6"/>
<connect gate="G$1" pin="BATT_VCC7" pad="7"/>
<connect gate="G$1" pin="BATT_VCC8" pad="8"/>
<connect gate="G$1" pin="BB_EMERGENCY_DWLD" pad="74"/>
<connect gate="G$1" pin="BB_JTAG_RTCK" pad="36"/>
<connect gate="G$1" pin="BB_JTAG_TCK" pad="26"/>
<connect gate="G$1" pin="BB_JTAG_TDI" pad="32"/>
<connect gate="G$1" pin="BB_JTAG_TDO" pad="30"/>
<connect gate="G$1" pin="BB_JTAG_TMS" pad="28"/>
<connect gate="G$1" pin="BB_UART_RXD" pad="66"/>
<connect gate="G$1" pin="BB_UART_TXD" pad="64"/>
<connect gate="G$1" pin="BB_USB_DN" pad="22"/>
<connect gate="G$1" pin="BB_USB_DP" pad="20"/>
<connect gate="G$1" pin="BB_USB_VBUS" pad="18"/>
<connect gate="G$1" pin="BT_UART_RXD" pad="21"/>
<connect gate="G$1" pin="BT_UART_TXD" pad="19"/>
<connect gate="G$1" pin="DEBUG_GPIO_LED" pad="72"/>
<connect gate="G$1" pin="FET_ON" pad="76"/>
<connect gate="G$1" pin="GND13" pad="13"/>
<connect gate="G$1" pin="GND16" pad="16"/>
<connect gate="G$1" pin="GND24" pad="24"/>
<connect gate="G$1" pin="GND27" pad="27"/>
<connect gate="G$1" pin="GND38" pad="38"/>
<connect gate="G$1" pin="GND55" pad="55"/>
<connect gate="G$1" pin="GND62" pad="62"/>
<connect gate="G$1" pin="GND69" pad="69"/>
<connect gate="G$1" pin="SIMCRD_CLK_CONN" pad="77"/>
<connect gate="G$1" pin="SIMCRD_IO_CONN" pad="79"/>
<connect gate="G$1" pin="SIMCRD_RST_CONN" pad="75"/>
<connect gate="G$1" pin="SIM_DETECT" pad="73"/>
<connect gate="G$1" pin="VREG_MSME" pad="9"/>
<connect gate="G$1" pin="VSIM_VAR" pad="71"/>
<connect gate="G$1" pin="WLAN_REG_ON" pad="17"/>
<connect gate="G$1" pin="WLAN_SDIO_CLK" pad="33"/>
<connect gate="G$1" pin="WLAN_SDIO_CMD" pad="35"/>
<connect gate="G$1" pin="WLAN_SDIO_DATA0" pad="43"/>
<connect gate="G$1" pin="WLAN_SDIO_DATA1" pad="41"/>
<connect gate="G$1" pin="WLAN_SDIO_DATA2" pad="39"/>
<connect gate="G$1" pin="WLAN_SDIO_DATA3" pad="37"/>
</connects>
<technologies>
<technology name=""/>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="FPC10">
<gates>
<gate name="G$1" symbol="PINHD10"/>
</gates>
<devices>
<device name="" package="FPC_SOLDER_10">
<connects>
<connect gate="G$1" pin="1" pad="1"/>
<connect gate="G$1" pin="10" pad="10"/>
<connect gate="G$1" pin="2" pad="2"/>
<connect gate="G$1" pin="3" pad="3"/>
<connect gate="G$1" pin="4" pad="4"/>
<connect gate="G$1" pin="5" pad="5"/>
<connect gate="G$1" pin="6" pad="6"/>
<connect gate="G$1" pin="7" pad="7"/>
<connect gate="G$1" pin="8" pad="8"/>
<connect gate="G$1" pin="9" pad="9"/>
</connects>
<technologies>
<technology name=""/>
</technologies>
</device>
<device name="J" package="TE184952-0">
<connects>
<connect gate="G$1" pin="1" pad="P$1"/>
<connect gate="G$1" pin="10" pad="P$10"/>
<connect gate="G$1" pin="2" pad="P$2"/>
<connect gate="G$1" pin="3" pad="P$3"/>
<connect gate="G$1" pin="4" pad="P$4"/>
<connect gate="G$1" pin="5" pad="P$5"/>
<connect gate="G$1" pin="6" pad="P$6"/>
<connect gate="G$1" pin="7" pad="P$7"/>
<connect gate="G$1" pin="8" pad="P$8"/>
<connect gate="G$1" pin="9" pad="P$9"/>
</connects>
<technologies>
<technology name=""/>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="FPC20">
<description>20pos FPC 0.5mm pitch / solder / socket</description>
<gates>
<gate name="G$1" symbol="PINHD20"/>
</gates>
<devices>
<device name="" package="FPC_SOLDER_20">
<connects>
<connect gate="G$1" pin="1" pad="1"/>
<connect gate="G$1" pin="10" pad="10"/>
<connect gate="G$1" pin="11" pad="11"/>
<connect gate="G$1" pin="12" pad="12"/>
<connect gate="G$1" pin="13" pad="13"/>
<connect gate="G$1" pin="14" pad="14"/>
<connect gate="G$1" pin="15" pad="15"/>
<connect gate="G$1" pin="16" pad="16"/>
<connect gate="G$1" pin="17" pad="17"/>
<connect gate="G$1" pin="18" pad="18"/>
<connect gate="G$1" pin="19" pad="19"/>
<connect gate="G$1" pin="2" pad="2"/>
<connect gate="G$1" pin="20" pad="20"/>
<connect gate="G$1" pin="3" pad="3"/>
<connect gate="G$1" pin="4" pad="4"/>
<connect gate="G$1" pin="5" pad="5"/>
<connect gate="G$1" pin="6" pad="6"/>
<connect gate="G$1" pin="7" pad="7"/>
<connect gate="G$1" pin="8" pad="8"/>
<connect gate="G$1" pin="9" pad="9"/>
</connects>
<technologies>
<technology name=""/>
</technologies>
</device>
<device name="J" package="SFV20R-1ST">
<connects>
<connect gate="G$1" pin="1" pad="1"/>
<connect gate="G$1" pin="10" pad="10"/>
<connect gate="G$1" pin="11" pad="11"/>
<connect gate="G$1" pin="12" pad="12"/>
<connect gate="G$1" pin="13" pad="13"/>
<connect gate="G$1" pin="14" pad="14"/>
<connect gate="G$1" pin="15" pad="15"/>
<connect gate="G$1" pin="16" pad="16"/>
<connect gate="G$1" pin="17" pad="17"/>
<connect gate="G$1" pin="18" pad="18"/>
<connect gate="G$1" pin="19" pad="19"/>
<connect gate="G$1" pin="2" pad="2"/>
<connect gate="G$1" pin="20" pad="20"/>
<connect gate="G$1" pin="3" pad="3"/>
<connect gate="G$1" pin="4" pad="4"/>
<connect gate="G$1" pin="5" pad="5"/>
<connect gate="G$1" pin="6" pad="6"/>
<connect gate="G$1" pin="7" pad="7"/>
<connect gate="G$1" pin="8" pad="8"/>
<connect gate="G$1" pin="9" pad="9"/>
</connects>
<technologies>
<technology name=""/>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="RDUP-880-915M-925-960M-4217-3W-S-J">
<description>Raditek Ceramic Duplexer 880-915MHz / 925-960MHz, Model 4216, 3 Watts, Surface Mount</description>
<gates>
<gate name="G$1" symbol="CER_DUP"/>
<gate name="G$2" symbol="RDUP_4217_GND"/>
</gates>
<devices>
<device name="" package="RADITEK_4217">
<connects>
<connect gate="G$1" pin="COM" pad="C"/>
<connect gate="G$1" pin="HI" pad="H"/>
<connect gate="G$1" pin="LO" pad="L"/>
<connect gate="G$2" pin="P$1" pad="G1"/>
<connect gate="G$2" pin="P$2" pad="G2"/>
<connect gate="G$2" pin="P$3" pad="G3"/>
<connect gate="G$2" pin="P$4" pad="G4"/>
<connect gate="G$2" pin="P$5" pad="G5"/>
<connect gate="G$2" pin="P$6" pad="G6"/>
<connect gate="G$2" pin="P$7" pad="G7"/>
</connects>
<technologies>
<technology name=""/>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="STC3100">
<description>ST STC3100 Battery monitor IC with coulomb counter/gas gauge</description>
<gates>
<gate name="G$1" symbol="STC3100"/>
</gates>
<devices>
<device name="" package="MINISO8">
<connects>
<connect gate="G$1" pin="CG" pad="6"/>
<connect gate="G$1" pin="GND" pad="5"/>
<connect gate="G$1" pin="IO0" pad="1"/>
<connect gate="G$1" pin="ROSC" pad="2"/>
<connect gate="G$1" pin="SCL" pad="4"/>
<connect gate="G$1" pin="SDA" pad="3"/>
<connect gate="G$1" pin="VCC" pad="7"/>
<connect gate="G$1" pin="VIN" pad="8"/>
</connects>
<technologies>
<technology name="">
<attribute name="OC_DIGIKEY" value="497-10526-1-ND"/>
</technology>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="BQ24160">
<description>2.5A, Dual-Input, Single ell Switchmode Li-Ion Battery Charger with Power Path Management and I2C Interface</description>
<gates>
<gate name="G$1" symbol="BQ2416X"/>
</gates>
<devices>
<device name="RGER" package="RGE_S_PVQFN_N24">
<connects>
<connect gate="G$1" pin="BAT" pad="11 12"/>
<connect gate="G$1" pin="BGATE" pad="10"/>
<connect gate="G$1" pin="BOOT" pad="19"/>
<connect gate="G$1" pin="CD" pad="24"/>
<connect gate="G$1" pin="DN" pad="1"/>
<connect gate="G$1" pin="DP" pad="2"/>
<connect gate="G$1" pin="DRV" pad="6"/>
<connect gate="G$1" pin="IN" pad="21"/>
<connect gate="G$1" pin="INT" pad="7"/>
<connect gate="G$1" pin="PGND" pad="5 15 16 17 THERMAL"/>
<connect gate="G$1" pin="PMIDI" pad="20"/>
<connect gate="G$1" pin="PMIDU" pad="23"/>
<connect gate="G$1" pin="SCL" pad="3"/>
<connect gate="G$1" pin="SDA" pad="4"/>
<connect gate="G$1" pin="STAT" pad="8"/>
<connect gate="G$1" pin="SW" pad="18"/>
<connect gate="G$1" pin="SYS" pad="13 14"/>
<connect gate="G$1" pin="TS" pad="9"/>
<connect gate="G$1" pin="USB" pad="22"/>
</connects>
<technologies>
<technology name="">
<attribute name="OC_DIGIKEY" value="296-30603-1-ND"/>
</technology>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="NR6828">
<description>Taio Yuden SMD Power Inductors (NR Series) NR6028</description>
<gates>
<gate name="L$1" symbol="L-EU"/>
</gates>
<devices>
<device name="" package="TY_NR_SERIES">
<connects>
<connect gate="L$1" pin="1" pad="P$1"/>
<connect gate="L$1" pin="2" pad="P$2"/>
</connects>
<technologies>
<technology name=""/>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="NCP380" prefix="IC">
<description>ONsemi NCP380, NCV380 Fixed/Adjustible Current-Limiting Power-Distribution Switches</description>
<gates>
<gate name="U$1" symbol="NCP380"/>
</gates>
<devices>
<device name="" package="TSOP-6">
<connects>
<connect gate="U$1" pin="!FLAG" pad="4"/>
<connect gate="U$1" pin="EN" pad="3"/>
<connect gate="U$1" pin="GND" pad="2"/>
<connect gate="U$1" pin="ILIM" pad="5"/>
<connect gate="U$1" pin="IN" pad="1"/>
<connect gate="U$1" pin="OUT" pad="6"/>
</connects>
<technologies>
<technology name=""/>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="IP4234CZ6" prefix="U">
<description>NXP IP4234CZ6 - Single USB 2.0 ESD protection to IEC 61000-4-2 level 4</description>
<gates>
<gate name="G$1" symbol="USB_TVS"/>
</gates>
<devices>
<device name="" package="TSOP-6">
<connects>
<connect gate="G$1" pin="1A" pad="1"/>
<connect gate="G$1" pin="1B" pad="3"/>
<connect gate="G$1" pin="2A" pad="6"/>
<connect gate="G$1" pin="2B" pad="4"/>
<connect gate="G$1" pin="GND" pad="2"/>
<connect gate="G$1" pin="VCC" pad="5"/>
</connects>
<technologies>
<technology name="">
<attribute name="OC_DIGIKEY" value="568-5869-1-ND"/>
</technology>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="PESD5V0UBV" prefix="D">
<description>NXP PESD5V0U5BV 5-channel bidirectional TVS array</description>
<gates>
<gate name="G$1" symbol="TVS_5_BIDIR"/>
</gates>
<devices>
<device name="" package="SOT666">
<connects>
<connect gate="G$1" pin="1" pad="1"/>
<connect gate="G$1" pin="2" pad="3"/>
<connect gate="G$1" pin="3" pad="4"/>
<connect gate="G$1" pin="4" pad="5"/>
<connect gate="G$1" pin="5" pad="6"/>
<connect gate="G$1" pin="GND" pad="2"/>
</connects>
<technologies>
<technology name="">
<attribute name="OC_DIGIKEY" value="568-7356-1-ND"/>
</technology>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="SSM3J130TU">
<description>Toshiba SSM3J130TU P-Type MOSFET</description>
<gates>
<gate name="Q$1" symbol="P_MOSFET"/>
</gates>
<devices>
<device name="" package="UFM">
<connects>
<connect gate="Q$1" pin="D" pad="P$3"/>
<connect gate="Q$1" pin="G" pad="P$1"/>
<connect gate="Q$1" pin="S" pad="P$2"/>
</connects>
<technologies>
<technology name="">
<attribute name="OC_DIGIKEY" value="SSM3J130TU(TE85L)CT-ND"/>
</technology>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="SN74LVC1G123">
<description>SN74LVC1G123 single retriggerable monostable multivibrator with schmitt-trigger inputs</description>
<gates>
<gate name="G$1" symbol="MONO_MULTIVIB"/>
</gates>
<devices>
<device name="" package="SSOP8">
<connects>
<connect gate="G$1" pin="A" pad="P$1"/>
<connect gate="G$1" pin="B" pad="P$2"/>
<connect gate="G$1" pin="C" pad="P$6"/>
<connect gate="G$1" pin="CLR" pad="P$3"/>
<connect gate="G$1" pin="GND" pad="P$4"/>
<connect gate="G$1" pin="Q" pad="P$5"/>
<connect gate="G$1" pin="R/C" pad="P$7"/>
<connect gate="G$1" pin="VCC" pad="P$8"/>
</connects>
<technologies>
<technology name="">
<attribute name="OC_DIGIKEY" value="296-18758-1-ND"/>
</technology>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="UEXT" prefix="X">
<description>UEXT header as used  by lots of Olimex designs</description>
<gates>
<gate name="G$1" symbol="UEXT"/>
</gates>
<devices>
<device name="" package="2X05">
<connects>
<connect gate="G$1" pin="3V3" pad="1"/>
<connect gate="G$1" pin="GND" pad="2"/>
<connect gate="G$1" pin="MISO" pad="7"/>
<connect gate="G$1" pin="MOSI" pad="8"/>
<connect gate="G$1" pin="RXD" pad="4"/>
<connect gate="G$1" pin="SCK" pad="9"/>
<connect gate="G$1" pin="SCL" pad="5"/>
<connect gate="G$1" pin="SDA" pad="6"/>
<connect gate="G$1" pin="SSEL" pad="10"/>
<connect gate="G$1" pin="TXD" pad="3"/>
</connects>
<technologies>
<technology name=""/>
</technologies>
</device>
<device name="/90" package="2X05/90">
<connects>
<connect gate="G$1" pin="3V3" pad="1"/>
<connect gate="G$1" pin="GND" pad="2"/>
<connect gate="G$1" pin="MISO" pad="7"/>
<connect gate="G$1" pin="MOSI" pad="8"/>
<connect gate="G$1" pin="RXD" pad="4"/>
<connect gate="G$1" pin="SCK" pad="9"/>
<connect gate="G$1" pin="SCL" pad="5"/>
<connect gate="G$1" pin="SDA" pad="6"/>
<connect gate="G$1" pin="SSEL" pad="10"/>
<connect gate="G$1" pin="TXD" pad="3"/>
</connects>
<technologies>
<technology name=""/>
</technologies>
</device>
<device name="/SMD/90" package="2X05_SMD_90">
<connects>
<connect gate="G$1" pin="3V3" pad="1"/>
<connect gate="G$1" pin="GND" pad="2"/>
<connect gate="G$1" pin="MISO" pad="7"/>
<connect gate="G$1" pin="MOSI" pad="8"/>
<connect gate="G$1" pin="RXD" pad="4"/>
<connect gate="G$1" pin="SCK" pad="9"/>
<connect gate="G$1" pin="SCL" pad="5"/>
<connect gate="G$1" pin="SDA" pad="6"/>
<connect gate="G$1" pin="SSEL" pad="10"/>
<connect gate="G$1" pin="TXD" pad="3"/>
</connects>
<technologies>
<technology name=""/>
</technologies>
</device>
<device name="/90-WUE" package="2X05/90-WUERTH">
<connects>
<connect gate="G$1" pin="3V3" pad="1"/>
<connect gate="G$1" pin="GND" pad="2"/>
<connect gate="G$1" pin="MISO" pad="7"/>
<connect gate="G$1" pin="MOSI" pad="8"/>
<connect gate="G$1" pin="RXD" pad="4"/>
<connect gate="G$1" pin="SCK" pad="9"/>
<connect gate="G$1" pin="SCL" pad="5"/>
<connect gate="G$1" pin="SDA" pad="6"/>
<connect gate="G$1" pin="SSEL" pad="10"/>
<connect gate="G$1" pin="TXD" pad="3"/>
</connects>
<technologies>
<technology name=""/>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="ELNA_DC_DCK_BAT">
<description>ELNA DC and DCK Super Cap

Tanken from data sheet of DCK-3R3E224U-E</description>
<gates>
<gate name="G$1" symbol="BATTERY2"/>
</gates>
<devices>
<device name="" package="ELNA_DC_E">
<connects>
<connect gate="G$1" pin="+" pad="+"/>
<connect gate="G$1" pin="-" pad="-"/>
</connects>
<technologies>
<technology name="">
<attribute name="OC_DIGIKEY" value="604-1007-ND"/>
</technology>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="MEDER_MK16">
<gates>
<gate name="G$1" symbol="REED_SWITCH"/>
</gates>
<devices>
<device name="" package="MK16">
<connects>
<connect gate="G$1" pin="1" pad="1"/>
<connect gate="G$1" pin="2" pad="2"/>
</connects>
<technologies>
<technology name="">
<attribute name="OC_DIGIKEY" value="374-1019-1-ND"/>
</technology>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="TPS389X">
<description>TI TPS3895, TPS3896, TPS3897, TPS3898
Single-Channel, Adjustable Supervisory Circuit in Ultra-Small Package</description>
<gates>
<gate name="G$1" symbol="TPS389X"/>
</gates>
<devices>
<device name="" package="USON6">
<connects>
<connect gate="G$1" pin="CT" pad="P5"/>
<connect gate="G$1" pin="EN" pad="P1"/>
<connect gate="G$1" pin="GND" pad="P2"/>
<connect gate="G$1" pin="OUT" pad="P4"/>
<connect gate="G$1" pin="SENSE" pad="P3"/>
<connect gate="G$1" pin="VCC" pad="P6"/>
</connects>
<technologies>
<technology name=""/>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="XB5353A">
<description>ysemi XB5353A One Cell Li-Ion/Li-Po Battery Protection IC</description>
<gates>
<gate name="G$1" symbol="YSEMI_BAT_PROT"/>
</gates>
<devices>
<device name="" package="SOT23L">
<connects>
<connect gate="G$1" pin="GND" pad="2"/>
<connect gate="G$1" pin="VDD" pad="3"/>
<connect gate="G$1" pin="VM" pad="4 5"/>
<connect gate="G$1" pin="VT" pad="1"/>
</connects>
<technologies>
<technology name=""/>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="UC530M">
<description>u-blox UC530M GNSS module</description>
<gates>
<gate name="G$1" symbol="UC530M"/>
</gates>
<devices>
<device name="" package="UC530M">
<connects>
<connect gate="G$1" pin="!RESET" pad="P$23"/>
<connect gate="G$1" pin="32K_DR_INT" pad="P$1"/>
<connect gate="G$1" pin="ANT" pad="P$16"/>
<connect gate="G$1" pin="EINT1" pad="P$7"/>
<connect gate="G$1" pin="FORCE_ON" pad="P$28"/>
<connect gate="G$1" pin="GND" pad="P$4 P$5 P$10 P$11 P$12 P$13 P$14 P$15 P$18 P$19 P$21 P$22 P$27 P$31"/>
<connect gate="G$1" pin="GPIO10" pad="P$24"/>
<connect gate="G$1" pin="GPIO9" pad="P$20"/>
<connect gate="G$1" pin="PPS" pad="P$29"/>
<connect gate="G$1" pin="RF_IN" pad="P$17"/>
<connect gate="G$1" pin="RX0" pad="P$26"/>
<connect gate="G$1" pin="RX1" pad="P$6"/>
<connect gate="G$1" pin="TX0" pad="P$25"/>
<connect gate="G$1" pin="TX1" pad="P$3"/>
<connect gate="G$1" pin="UI_FIX" pad="P$2"/>
<connect gate="G$1" pin="VDD" pad="P$9"/>
<connect gate="G$1" pin="VDD_B" pad="P$8"/>
<connect gate="G$1" pin="WAKEUP" pad="P$30"/>
</connects>
<technologies>
<technology name=""/>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="NC7SZ125" prefix="IC">
<description>Fairchild TinyLogic NC7SZ125 UHS Buffer with Three-State Output</description>
<gates>
<gate name="-1" symbol="74*125"/>
<gate name="-P" symbol="PWRN"/>
</gates>
<devices>
<device name="" package="SOT23L">
<connects>
<connect gate="-1" pin="I" pad="2"/>
<connect gate="-1" pin="O" pad="4"/>
<connect gate="-1" pin="OE" pad="1"/>
<connect gate="-P" pin="GND" pad="3"/>
<connect gate="-P" pin="VCC" pad="5"/>
</connects>
<technologies>
<technology name="">
<attribute name="OC_DIGIKEY" value="NC7SZ125M5XCT-ND"/>
</technology>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="AMP_MINICT_1X5">
<description>AMP Mini CT Connector 1.5mm PITCH 292228-5</description>
<gates>
<gate name="X$1" symbol="PINHD5"/>
</gates>
<devices>
<device name="" package="29228-5">
<connects>
<connect gate="X$1" pin="1" pad="1"/>
<connect gate="X$1" pin="2" pad="2"/>
<connect gate="X$1" pin="3" pad="3"/>
<connect gate="X$1" pin="4" pad="4"/>
<connect gate="X$1" pin="5" pad="5"/>
</connects>
<technologies>
<technology name="">
<attribute name="OC_DIGIKEY" value="A101010CT-ND"/>
</technology>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="SMA-F" prefix="X" uservalue="yes">
<gates>
<gate name="G" symbol="COAX-F-4GND"/>
</gates>
<devices>
<device name="-S-EDGE" package="SMA-F-S-EDGE">
<connects>
<connect gate="G" pin="1" pad="C"/>
<connect gate="G" pin="GND@1" pad="BG1"/>
<connect gate="G" pin="GND@2" pad="TG1"/>
<connect gate="G" pin="GND@3" pad="TG2"/>
<connect gate="G" pin="GND@4" pad="BG2"/>
</connects>
<technologies>
<technology name=""/>
</technologies>
</device>
<device name="-S-TH" package="SMA-F-S-TH">
<connects>
<connect gate="G" pin="1" pad="C"/>
<connect gate="G" pin="GND@1" pad="G1"/>
<connect gate="G" pin="GND@2" pad="G2"/>
<connect gate="G" pin="GND@3" pad="G3"/>
<connect gate="G" pin="GND@4" pad="G4"/>
</connects>
<technologies>
<technology name=""/>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="L-EU" prefix="L" uservalue="yes">
<description>Inductors</description>
<gates>
<gate name="G$1" symbol="L-EU"/>
</gates>
<devices>
<device name="-TY-NR" package="TY_NR_SERIES">
<connects>
<connect gate="G$1" pin="1" pad="P$1"/>
<connect gate="G$1" pin="2" pad="P$2"/>
</connects>
<technologies>
<technology name=""/>
</technologies>
</device>
<device name="-1210" package="L1210">
<connects>
<connect gate="G$1" pin="1" pad="1"/>
<connect gate="G$1" pin="2" pad="2"/>
</connects>
<technologies>
<technology name=""/>
</technologies>
</device>
<device name="-IFSC-1515AH" package="IFSC-1515AH">
<connects>
<connect gate="G$1" pin="1" pad="P$1"/>
<connect gate="G$1" pin="2" pad="P$2"/>
</connects>
<technologies>
<technology name=""/>
</technologies>
</device>
<device name="-SRN1060" package="SRN1060">
<connects>
<connect gate="G$1" pin="1" pad="1"/>
<connect gate="G$1" pin="2" pad="2"/>
</connects>
<technologies>
<technology name=""/>
</technologies>
</device>
<device name="-CDRH4D28" package="CDRH4D28">
<connects>
<connect gate="G$1" pin="1" pad="1"/>
<connect gate="G$1" pin="2" pad="2"/>
</connects>
<technologies>
<technology name=""/>
</technologies>
</device>
<device name="-SRP1250" package="SRP1250">
<connects>
<connect gate="G$1" pin="1" pad="1"/>
<connect gate="G$1" pin="2" pad="2"/>
</connects>
<technologies>
<technology name=""/>
</technologies>
</device>
<device name="-0402" package="AISC0402">
<connects>
<connect gate="G$1" pin="1" pad="1"/>
<connect gate="G$1" pin="2" pad="2"/>
</connects>
<technologies>
<technology name=""/>
</technologies>
</device>
<device name="-0603" package="0603">
<connects>
<connect gate="G$1" pin="1" pad="1"/>
<connect gate="G$1" pin="2" pad="2"/>
</connects>
<technologies>
<technology name=""/>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="D-ZENER" prefix="ZD" uservalue="yes">
<gates>
<gate name="G$1" symbol="D-ZENER"/>
</gates>
<devices>
<device name="-SOD323" package="SOD323">
<connects>
<connect gate="G$1" pin="A" pad="2A"/>
<connect gate="G$1" pin="C" pad="1C"/>
</connects>
<technologies>
<technology name=""/>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="USB-A" prefix="X">
<description>USB A socket THT Amphenol UE27-AEX4-X0X</description>
<gates>
<gate name="G$1" symbol="USB-A"/>
</gates>
<devices>
<device name="-VERT" package="USB_A_VERT">
<connects>
<connect gate="G$1" pin="D_N" pad="2"/>
<connect gate="G$1" pin="D_P" pad="3"/>
<connect gate="G$1" pin="GND" pad="4"/>
<connect gate="G$1" pin="SHIELD" pad="P$1 P$2"/>
<connect gate="G$1" pin="VBUS" pad="1"/>
</connects>
<technologies>
<technology name=""/>
</technologies>
</device>
<device name="-HORIZ" package="USB_A_HORIZ">
<connects>
<connect gate="G$1" pin="D_N" pad="2"/>
<connect gate="G$1" pin="D_P" pad="3"/>
<connect gate="G$1" pin="GND" pad="4"/>
<connect gate="G$1" pin="SHIELD" pad="P$1 P$2"/>
<connect gate="G$1" pin="VBUS" pad="1"/>
</connects>
<technologies>
<technology name=""/>
</technologies>
</device>
<device name="-MALE" package="USB-A-MALE">
<connects>
<connect gate="G$1" pin="D_N" pad="2"/>
<connect gate="G$1" pin="D_P" pad="3"/>
<connect gate="G$1" pin="GND" pad="4"/>
<connect gate="G$1" pin="SHIELD" pad="S1 S2"/>
<connect gate="G$1" pin="VBUS" pad="1"/>
</connects>
<technologies>
<technology name=""/>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="USB-A-VERT" prefix="X">
<description>Amphenol UE27-AEX4-X0X</description>
<gates>
<gate name="G$1" symbol="USB-A"/>
</gates>
<devices>
<device name="" package="USB_A_VERT">
<connects>
<connect gate="G$1" pin="D_N" pad="2"/>
<connect gate="G$1" pin="D_P" pad="3"/>
<connect gate="G$1" pin="GND" pad="4"/>
<connect gate="G$1" pin="SHIELD" pad="P$1 P$2"/>
<connect gate="G$1" pin="VBUS" pad="1"/>
</connects>
<technologies>
<technology name=""/>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="MOSFET-N" prefix="Q">
<description>Rohm RSQ045N03</description>
<gates>
<gate name="G$1" symbol="MOSFET-N"/>
</gates>
<devices>
<device name="-SOT236" package="SOT23-6">
<connects>
<connect gate="G$1" pin="D" pad="1 2 5 6"/>
<connect gate="G$1" pin="G" pad="3"/>
<connect gate="G$1" pin="S" pad="4"/>
</connects>
<technologies>
<technology name=""/>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="MOSFET-P" prefix="Q">
<description>P-Channel MOSFET in SOT23-6 case, Example: Diodes DMP2066LDM</description>
<gates>
<gate name="G$1" symbol="P_MOSFET"/>
</gates>
<devices>
<device name="" package="SOT23-6">
<connects>
<connect gate="G$1" pin="D" pad="1 2 5 6"/>
<connect gate="G$1" pin="G" pad="3"/>
<connect gate="G$1" pin="S" pad="4"/>
</connects>
<technologies>
<technology name=""/>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="SUPPRESSOR-" prefix="D" uservalue="yes">
<gates>
<gate name="G$1" symbol="SUPPRESSOR"/>
</gates>
<devices>
<device name="SMBJ" package="SMBJ">
<connects>
<connect gate="G$1" pin="A" pad="A"/>
<connect gate="G$1" pin="C" pad="C"/>
</connects>
<technologies>
<technology name=""/>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="TRS3232E" prefix="U">
<gates>
<gate name="G$1" symbol="TRS3232E"/>
</gates>
<devices>
<device name="CPW" package="TSSOP16">
<connects>
<connect gate="G$1" pin="C1N" pad="3"/>
<connect gate="G$1" pin="C1P" pad="1"/>
<connect gate="G$1" pin="C2N" pad="5"/>
<connect gate="G$1" pin="C2P" pad="4"/>
<connect gate="G$1" pin="GND" pad="15"/>
<connect gate="G$1" pin="R1IN" pad="13"/>
<connect gate="G$1" pin="R1OUT" pad="12"/>
<connect gate="G$1" pin="R2IN" pad="8"/>
<connect gate="G$1" pin="R2OUT" pad="9"/>
<connect gate="G$1" pin="T1IN" pad="11"/>
<connect gate="G$1" pin="T1OUT" pad="14"/>
<connect gate="G$1" pin="T2IN" pad="10"/>
<connect gate="G$1" pin="T2OUT" pad="7"/>
<connect gate="G$1" pin="VCC" pad="16"/>
<connect gate="G$1" pin="VN" pad="6"/>
<connect gate="G$1" pin="VP" pad="2"/>
</connects>
<technologies>
<technology name=""/>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="XTAL-SHIELD" prefix="Q" uservalue="yes">
<gates>
<gate name="G$1" symbol="Q-SHIELD"/>
</gates>
<devices>
<device name="-ABM10" package="ABRACON_ABM10">
<connects>
<connect gate="G$1" pin="1" pad="1"/>
<connect gate="G$1" pin="2" pad="3"/>
<connect gate="G$1" pin="GND1" pad="2"/>
<connect gate="G$1" pin="GND2" pad="4"/>
</connects>
<technologies>
<technology name=""/>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="XTAL" prefix="Q" uservalue="yes">
<gates>
<gate name="G$1" symbol="Q"/>
</gates>
<devices>
<device name="-ABM3" package="ABM3">
<connects>
<connect gate="G$1" pin="1" pad="1"/>
<connect gate="G$1" pin="2" pad="2"/>
</connects>
<technologies>
<technology name=""/>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="PINHD-2X8" prefix="X">
<description>PIN HEADER</description>
<gates>
<gate name="G$1" symbol="PINH2X8"/>
</gates>
<devices>
<device name="" package="2X08_SMD_180">
<connects>
<connect gate="G$1" pin="1" pad="1"/>
<connect gate="G$1" pin="10" pad="10"/>
<connect gate="G$1" pin="11" pad="11"/>
<connect gate="G$1" pin="12" pad="12"/>
<connect gate="G$1" pin="13" pad="13"/>
<connect gate="G$1" pin="14" pad="14"/>
<connect gate="G$1" pin="15" pad="15"/>
<connect gate="G$1" pin="16" pad="16"/>
<connect gate="G$1" pin="2" pad="2"/>
<connect gate="G$1" pin="3" pad="3"/>
<connect gate="G$1" pin="4" pad="4"/>
<connect gate="G$1" pin="5" pad="5"/>
<connect gate="G$1" pin="6" pad="6"/>
<connect gate="G$1" pin="7" pad="7"/>
<connect gate="G$1" pin="8" pad="8"/>
<connect gate="G$1" pin="9" pad="9"/>
</connects>
<technologies>
<technology name=""/>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="PINHD-2X2" prefix="X">
<gates>
<gate name="G$1" symbol="PINH2X2"/>
</gates>
<devices>
<device name="" package="2X02_SMD_180">
<connects>
<connect gate="G$1" pin="1" pad="1"/>
<connect gate="G$1" pin="2" pad="2"/>
<connect gate="G$1" pin="3" pad="3"/>
<connect gate="G$1" pin="4" pad="4"/>
</connects>
<technologies>
<technology name=""/>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="PINHD-2X3" prefix="X">
<gates>
<gate name="G$1" symbol="PINH2X3"/>
</gates>
<devices>
<device name="" package="2X03_SMD_180">
<connects>
<connect gate="G$1" pin="1" pad="1"/>
<connect gate="G$1" pin="2" pad="2"/>
<connect gate="G$1" pin="3" pad="3"/>
<connect gate="G$1" pin="4" pad="4"/>
<connect gate="G$1" pin="5" pad="5"/>
<connect gate="G$1" pin="6" pad="6"/>
</connects>
<technologies>
<technology name=""/>
</technologies>
</device>
<device name="-SP" package="2X03_SMD_180_SP">
<connects>
<connect gate="G$1" pin="1" pad="1"/>
<connect gate="G$1" pin="2" pad="2"/>
<connect gate="G$1" pin="3" pad="3"/>
<connect gate="G$1" pin="4" pad="4"/>
<connect gate="G$1" pin="5" pad="5"/>
<connect gate="G$1" pin="6" pad="6"/>
</connects>
<technologies>
<technology name=""/>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="PINHD-1X5">
<gates>
<gate name="G$1" symbol="PINHD5"/>
</gates>
<devices>
<device name="" package="1X05_SMD">
<connects>
<connect gate="G$1" pin="1" pad="1"/>
<connect gate="G$1" pin="2" pad="2"/>
<connect gate="G$1" pin="3" pad="3"/>
<connect gate="G$1" pin="4" pad="4"/>
<connect gate="G$1" pin="5" pad="5"/>
</connects>
<technologies>
<technology name=""/>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="74AVC1T45" prefix="IC">
<description>single-bit dual-supply bus transceiver with configurable voltage translation and 3-state outputs</description>
<gates>
<gate name="G$1" symbol="74*1T45"/>
</gates>
<devices>
<device name="" package="SOT23-6">
<connects>
<connect gate="G$1" pin="1A" pad="3"/>
<connect gate="G$1" pin="1B" pad="4"/>
<connect gate="G$1" pin="DIR" pad="5"/>
<connect gate="G$1" pin="GND" pad="2"/>
<connect gate="G$1" pin="VCC_A" pad="1"/>
<connect gate="G$1" pin="VCC_B" pad="6"/>
</connects>
<technologies>
<technology name=""/>
</technologies>
</device>
<device name="GW" package="SOT363">
<connects>
<connect gate="G$1" pin="1A" pad="3"/>
<connect gate="G$1" pin="1B" pad="4"/>
<connect gate="G$1" pin="DIR" pad="5"/>
<connect gate="G$1" pin="GND" pad="2"/>
<connect gate="G$1" pin="VCC_A" pad="1"/>
<connect gate="G$1" pin="VCC_B" pad="6"/>
</connects>
<technologies>
<technology name=""/>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="PINHD-1X3" prefix="X" uservalue="yes">
<description>&lt;b&gt;Header 3&lt;/b&gt;
Standard 3-pin 0.1" header</description>
<gates>
<gate name="G$1" symbol="M03"/>
</gates>
<devices>
<device name="LOCK" package="1X03_LOCK">
<connects>
<connect gate="G$1" pin="1" pad="1"/>
<connect gate="G$1" pin="2" pad="2"/>
<connect gate="G$1" pin="3" pad="3"/>
</connects>
<technologies>
<technology name=""/>
</technologies>
</device>
<device name="LOCK_LONGPADS" package="1X03_LOCK_LONGPADS">
<connects>
<connect gate="G$1" pin="1" pad="1"/>
<connect gate="G$1" pin="2" pad="2"/>
<connect gate="G$1" pin="3" pad="3"/>
</connects>
<technologies>
<technology name=""/>
</technologies>
</device>
<device name="LOCK_NO_SILK" package="1X03_LOCK_NO_SILK">
<connects>
<connect gate="G$1" pin="1" pad="1"/>
<connect gate="G$1" pin="2" pad="2"/>
<connect gate="G$1" pin="3" pad="3"/>
</connects>
<technologies>
<technology name=""/>
</technologies>
</device>
<device name="PTH" package="1X03">
<connects>
<connect gate="G$1" pin="1" pad="1"/>
<connect gate="G$1" pin="2" pad="2"/>
<connect gate="G$1" pin="3" pad="3"/>
</connects>
<technologies>
<technology name=""/>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="NC7SZ126" prefix="IC">
<gates>
<gate name="-1" symbol="74*126"/>
<gate name="-P" symbol="PWRN"/>
</gates>
<devices>
<device name="" package="SOT23L">
<connects>
<connect gate="-1" pin="I" pad="2"/>
<connect gate="-1" pin="O" pad="4"/>
<connect gate="-1" pin="OE" pad="1"/>
<connect gate="-P" pin="GND" pad="3"/>
<connect gate="-P" pin="VCC" pad="5"/>
</connects>
<technologies>
<technology name=""/>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="PULSE_T1094NL" prefix="TR">
<gates>
<gate name="-1:1" symbol="E1_MAGNETICS"/>
<gate name="-1:2" symbol="E1_MAGNETICS"/>
</gates>
<devices>
<device name="" package="PULSE_BH">
<connects>
<connect gate="-1:1" pin="P$1" pad="16"/>
<connect gate="-1:1" pin="P$2" pad="15"/>
<connect gate="-1:1" pin="P$3" pad="14"/>
<connect gate="-1:1" pin="P$4" pad="1"/>
<connect gate="-1:1" pin="P$5" pad="2"/>
<connect gate="-1:1" pin="P$6" pad="3"/>
<connect gate="-1:2" pin="P$1" pad="11"/>
<connect gate="-1:2" pin="P$2" pad="10"/>
<connect gate="-1:2" pin="P$3" pad="9"/>
<connect gate="-1:2" pin="P$4" pad="6"/>
<connect gate="-1:2" pin="P$5" pad="7"/>
<connect gate="-1:2" pin="P$6" pad="8"/>
</connects>
<technologies>
<technology name=""/>
</technologies>
</device>
</devices>
</deviceset>
</devicesets>
</library>
</drawing>
</eagle>
