<?xml version="1.0" encoding="utf-8"?>
<!DOCTYPE eagle SYSTEM "eagle.dtd">
<eagle version="6.4">
<drawing>
<library>
<packages>
<package name="UMAX8">
<description>&lt;b&gt;micro MAX Package&lt;/b&gt;</description>
</package>
</packages>
<symbols>
<symbol name="MAX521X">
<description>DAC w/ I²C</description>
<pin name="VREF" direction="in"/>
<pin name="OUT" direction="out"/>
<pin name="GND" direction="pwr"/>
<pin name="SCL" direction="in"/>
<pin name="SDA"/>
<pin name="ADDR" direction="in"/>
<pin name="!AUX" direction="in"/>
<pin name="VDD" direction="pwr"/>
</symbol>
</symbols>
<devicesets>
<deviceset name="MAX521" prefix="IC">
<description>&lt;b&gt;MAX5215/MAX5217
14-/16-Bit, Low-Power, Buffered Output,
Rail-to-Rail DACs with I²C Interface&lt;/b&gt;</description>
<gates>
<gate name="G$1" symbol="MAX521X"/>
</gates>
<devices>
<device name="" package="UMAX8">
<connects>
<connect gate="G$1" pin="!AUX" pad="5"/>
<connect gate="G$1" pin="ADDR" pad="2"/>
<connect gate="G$1" pin="GND" pad="8"/>
<connect gate="G$1" pin="OUT" pad="6"/>
<connect gate="G$1" pin="SCL" pad="3"/>
<connect gate="G$1" pin="SDA" pad="4"/>
<connect gate="G$1" pin="VDD" pad="7"/>
<connect gate="G$1" pin="VREF" pad="1"/>
</connects>
<technologies>
<technology name="5"/>
</technologies>
</device>
</devices>
</deviceset>
</devicesets>
</library>
</drawing>
</eagle>
